# BMA456 Sensor API

> This package contains SensorAPIs for BMA456 Sensor

## Sensor Overview

The BMA456 is an ultra-small, triaxial, low-g acceleration sensor with digital interfaces, aiming for low-power consumer electronics applications. Featuring 16 bit digital resolution and embedded intelligence, the device is optimized to fulfill low power accelerometer requirements.

## Applications

### BMA456W
- Any motion
- No motion 
- Step detector
- Step counter
- Step activity
- Tap
	- Single tap
	- Double tap

### BMA456H

- Any motion
- No motion 
- Step detector
- Step counter
- Step activity
- Auto low power
- Tap
	- Single tap
	- Double tap
	- Triple tap

### BMA456MM

- Any motion
- No motion 
- Orientation
- High-g
- Low-g
- Significant motion
- Auto low power
- Tap
	- Single tap
	- Double tap
	- Triple tap

### BMA456AN

- Any motion
- No motion

### BMA456 tablet

- Any/no motion 
- Low-g
- Single, double and triple tap
- Orientation