SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

UserSettings.h
Go to the documentation of this file.
1 /*
2 MIT License
3
4 Copyright (c) 2018, Alexey Dynda
5
6 Permission is hereby granted, free of charge, to any person obtaining a copy
7 of this software and associated documentation files (the "Software"), to deal
8 in the Software without restriction, including without limitation the rights
9 to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
10 copies of the Software, and to permit persons to whom the Software is
11 furnished to do so, subject to the following conditions:
12
13 The above copyright notice and this permission notice shall be included in all
14 copies or substantial portions of the Software.
15
16 THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
17 IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
18 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
19 AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
20 LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
21 OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
22 SOFTWARE.
23 */
28 #ifndef _USER_SETTINGS_H_
29 #define _USER_SETTINGS_H_
30
48 /* Comment out options below if you don't need support in the library, *
49 * and want to reduce memory consumption. */
50
52 #define CONFIG_SOFTWARE_I2C_ENABLE
53
55 #define CONFIG_TWI_I2C_ENABLE
56
58 #define CONFIG_AVR_SPI_ENABLE
59
61 #define CONFIG_USI_SPI_ENABLE
62
64 #define CONFIG_AVR_UART_ENABLE
65
67 #define CONFIG_VGA_ENABLE
68
70 #ifndef CONFIG_ADAFRUIT_GFX_ENABLE
71 //#define CONFIG_ADAFRUIT_GFX_ENABLE
72 #endif
73
78 #define CONFIG_PLATFORM_I2C_ENABLE
79
84 #define CONFIG_PLATFORM_SPI_ENABLE
85
90 #define CONFIG_SSD1306_UNICODE_ENABLE
91
96 #endif