SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

adafruit.h
Go to the documentation of this file.
1 /*
2 MIT License
3
4 Copyright (c) 2018, Alexey Dynda
5
6 Permission is hereby granted, free of charge, to any person obtaining a copy
7 of this software and associated documentation files (the "Software"), to deal
8 in the Software without restriction, including without limitation the rights
9 to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
10 copies of the Software, and to permit persons to whom the Software is
11 furnished to do so, subject to the following conditions:
12
13 The above copyright notice and this permission notice shall be included in all
14 copies or substantial portions of the Software.
15
16 THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
17 IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
18 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
19 AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
20 LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
21 OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
22 SOFTWARE.
23 */
35 #ifndef _SSD1306_ADAFRUIT_H_
36 #define _SSD1306_ADAFRUIT_H_
37
38 #include "ssd1306_hal/io.h"
39
40 #if defined(CONFIG_ADAFRUIT_GFX_ENABLE)
41
42 #include "ssd1306.h"
43 #include "ssd1306_hal/Print_internal.h"
44 #include "nano_gfx_types.h"
45
46 #ifndef DOXYGEN_SHOULD_SKIP_THIS
47 /* This is special case for non-Arduino platforms, since Adafruit requires *
48 * Arduino libraries support */
49 #ifndef ARDUINO
50 #define ARDUINO 100
51 #include "Adafruit_GFX.h"
52 #undef ARDUINO
53 #else
54 #include "Adafruit_GFX.h"
55 #endif
56
57 #endif // DOXYGEN_SHOULD_SKIP_THIS
58
70 template <uint8_t BPP>
71 class AdafruitCanvasOps: public Adafruit_GFX
72 {
73 public:
75 NanoPoint offset;
76
78 static const uint8_t BITS_PER_PIXEL = BPP;
79
88 AdafruitCanvasOps(lcduint_t w, lcduint_t h, uint8_t *buffer)
89 : Adafruit_GFX(w, h)
90 , offset{0}
91 , m_buffer(buffer)
92 {
93 }
94
103 void drawPixel(int16_t x, int16_t y, uint16_t color) override;
104
110 void setOffset(lcdint_t ox, lcdint_t oy) { offset.x = ox; offset.y = oy; };
111
112 #ifndef DOXYGEN_SHOULD_SKIP_THIS
113 // We need to override Adafruit GFX implementation of fillScreen, because
114 // NanoEngine uses offsets, when refreshing screen content.
115 void fillScreen(uint16_t color) override
116 {
117 fillRect(offset.x, offset.y, _width, _height, color);
118 }
119 #endif
120
121 protected:
122
124 uint8_t *m_buffer;
125
126 private:
127 inline void rotatePosition(int16_t &x, int16_t &y)
128 {
129 switch (getRotation()) {
130 case 1:
131 ssd1306_swap_data(x, y, int16_t);
132 x = WIDTH - x - 1;
133 break;
134 case 2:
135 x = WIDTH - x - 1;
136 y = HEIGHT - y - 1;
137 break;
138 case 3:
139 ssd1306_swap_data(x, y, int16_t);
140 y = HEIGHT - y - 1;
141 break;
142 }
143
144 }
145 };
146
150 template <uint8_t BPP>
151 class AdafruitCanvasBase: public AdafruitCanvasOps<BPP>
152 {
153 public:
154 using AdafruitCanvasOps<BPP>::AdafruitCanvasOps;
155
161 virtual void blt(lcdint_t x, lcdint_t y) = 0;
162
166 virtual void blt() = 0;
167 };
168
170 //
171 // 1-BIT GRAPHICS
172 //
174
180 class AdafruitCanvas1 : public AdafruitCanvasBase<1>
181 {
182 public:
183 using AdafruitCanvasBase::AdafruitCanvasBase;
184
190 void blt(lcdint_t x, lcdint_t y) override
191 {
192 ssd1306_drawBufferFast(x, y, WIDTH, HEIGHT, m_buffer);
193 }
194
198 void blt() override
199 {
200 ssd1306_drawBufferFast(offset.x, offset.y, WIDTH, HEIGHT, m_buffer);
201 }
202 };
203
204 #ifndef DOXYGEN_SHOULD_SKIP_THIS
205 template <>
206 void AdafruitCanvasOps<1>::drawPixel(int16_t x, int16_t y, uint16_t color)
207 {
208 x -= offset.x;
209 y -= offset.y;
210 if ((x < 0) || (x >= width()) || (y < 0) || (y >= height()))
211 {
212 return;
213 }
214 rotatePosition(x, y);
215
216 switch (color)
217 {
218 case 1: m_buffer[x+ (y/8)*WIDTH] |= (1 << (y&7)); break;
219 case 0: m_buffer[x+ (y/8)*WIDTH] &= ~(1 << (y&7)); break;
220 case 2: m_buffer[x+ (y/8)*WIDTH] ^= (1 << (y&7)); break;
221 }
222 }
223 #endif // DOXYGEN_SHOULD_SKIP_THIS
224
226 //
227 // 8-BIT GRAPHICS
228 //
230
236 class AdafruitCanvas8 : public AdafruitCanvasBase<8>
237 {
238 public:
239 using AdafruitCanvasBase::AdafruitCanvasBase;
240
246 void blt(lcdint_t x, lcdint_t y) override
247 {
248 ssd1306_drawBufferFast8(x, y, WIDTH, HEIGHT, m_buffer);
249 }
250
254 void blt() override
255 {
256 ssd1306_drawBufferFast8(offset.x, offset.y, WIDTH, HEIGHT, m_buffer);
257 }
258 };
259
260 #ifndef DOXYGEN_SHOULD_SKIP_THIS
261 template <>
262 void AdafruitCanvasOps<8>::drawPixel(int16_t x, int16_t y, uint16_t color)
263 {
264 x -= offset.x;
265 y -= offset.y;
266 if ((x < 0) || (x >= width()) || (y < 0) || (y >= height()))
267 {
268 return;
269 }
270 rotatePosition(x, y);
271
272 m_buffer[x+y*WIDTH] = color;
273 }
274 #endif // DOXYGEN_SHOULD_SKIP_THIS
275
277 //
278 // 16-BIT GRAPHICS
279 //
281
288 class AdafruitCanvas16 : public AdafruitCanvasBase<16>
289 {
290 public:
291 using AdafruitCanvasBase::AdafruitCanvasBase;
292
298 void blt(lcdint_t x, lcdint_t y) override
299 {
300 ssd1306_drawBufferFast16(x, y, WIDTH, HEIGHT, m_buffer);
301 }
302
306 void blt() override
307 {
308 ssd1306_drawBufferFast16(offset.x, offset.y, WIDTH, HEIGHT, m_buffer);
309 }
310 };
311
312 #ifndef DOXYGEN_SHOULD_SKIP_THIS
313 template <>
314 void AdafruitCanvasOps<16>::drawPixel(int16_t x, int16_t y, uint16_t color)
315 {
316 x -= offset.x;
317 y -= offset.y;
318 if ((x < 0) || (x >= width()) || (y < 0) || (y >= height()))
319 {
320 return;
321 }
322 rotatePosition(x, y);
323
324 m_buffer[(x+y*WIDTH) * 2 + 0] = color;
325 m_buffer[(x+y*WIDTH) * 2 + 1] = color >> 8;
326 }
327 #endif // DOXYGEN_SHOULD_SKIP_THIS
328
333 #endif // CONFIG_ADAFRUIT_GFX_ENABLE
334
335 #endif
AdafruitCanvasOps::AdafruitCanvasOps
AdafruitCanvasOps(lcduint_t w, lcduint_t h, uint8_t *buffer)
Definition: adafruit.h:88
AdafruitCanvas1::blt
void blt() override
Definition: adafruit.h:198
AdafruitCanvas16::blt
void blt(lcdint_t x, lcdint_t y) override
Definition: adafruit.h:298
_NanoPoint
Definition: point.h:40
ssd1306.h
AdafruitCanvasOps::setOffset
void setOffset(lcdint_t ox, lcdint_t oy)
Definition: adafruit.h:110
AdafruitCanvasOps
Definition: adafruit.h:71
io.h
AdafruitCanvas1
Definition: adafruit.h:180
AdafruitCanvas16
Definition: adafruit.h:288
_NanoPoint::y
lcdint_t y
Definition: point.h:45
AdafruitCanvasBase
Definition: adafruit.h:151
AdafruitCanvas8
Definition: adafruit.h:236
ssd1306_drawBufferFast16
void ssd1306_drawBufferFast16(lcdint_t x, lcdint_t y, lcduint_t w, lcduint_t h, const uint8_t *data)
Definition: ssd1306_16bit.c:61
Print_internal.h
AdafruitCanvasOps::m_buffer
uint8_t * m_buffer
Definition: adafruit.h:110
nano_gfx_types.h
AdafruitCanvasOps::BITS_PER_PIXEL
static const uint8_t BITS_PER_PIXEL
Definition: adafruit.h:78
AdafruitCanvas16::blt
void blt() override
Definition: adafruit.h:306
ssd1306_drawBufferFast8
void ssd1306_drawBufferFast8(lcdint_t x, lcdint_t y, lcduint_t w, lcduint_t h, const uint8_t *data)
Definition: ssd1306_8bit.c:106
AdafruitCanvas8::blt
void blt(lcdint_t x, lcdint_t y) override
Definition: adafruit.h:246
AdafruitCanvas8::blt
void blt() override
Definition: adafruit.h:254
_NanoPoint::x
lcdint_t x
Definition: point.h:43
AdafruitCanvas1::blt
void blt(lcdint_t x, lcdint_t y) override
Definition: adafruit.h:190
ssd1306_drawBufferFast
void ssd1306_drawBufferFast(lcdint_t x, lcdint_t y, lcduint_t w, lcduint_t h, const uint8_t *buf)
Definition: ssd1306_1bit.c:725
AdafruitCanvasOps::drawPixel
void drawPixel(int16_t x, int16_t y, uint16_t color) override
ssd1306_swap_data
#define ssd1306_swap_data(a, b, type)
Definition: io.h:69
AdafruitCanvasOps::offset
NanoPoint offset
Definition: adafruit.h:75