SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Functions
oled_ssd1331.h File Reference
`#include "ssd1306_hal/io.h"`
`#include "lcd/lcd_common.h"`

Go to the source code of this file.

## Functions
void | ssd1331_setRotation (uint8_t rotation)
| Sets screen orientation (rotation) More...
void | ssd1331_setMode (lcd_mode_t mode)
| Sets GDRAM autoincrement mode. More...
void | ssd1331_96x64_init (void)
| Inits 96x64 RGB OLED display (based on SSD1331 controller). More...
void | ssd1331_96x64_spi_init (int8_t rstPin, int8_t cesPin, int8_t dcPin)
| Inits 96x64 RGB OLED display over spi in 8-bit mode (based on SSD1331 controller). More...
void | ssd1331_96x64_spi_init16 (int8_t rstPin, int8_t cesPin, int8_t dcPin)
| Inits 96x64 RGB OLED display over spi in 16-bit mode (based on SSD1331 controller). More...
void | ssd1331_drawLine (uint8_t x1, uint8_t y1, uint8_t x2, uint8_t y2, uint16_t color)
void | ssd1331_copyBlock (uint8_t left, uint8_t top, uint8_t right, uint8_t bottom, uint8_t newLeft, uint8_t newTop)

## Detailed Description

support for RGB OLED 96x64 display

Definition in file oled_ssd1331.h.