SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Functions
ili9341: ili9341 control functions

## Functions
void | ili9341_setRotation (uint8_t rotation)
| Sets screen orientation (rotation) More...
void | ili9341_rotateOutput (uint8_t on)
| Sets rotation of all output functions. More...

## Detailed Description

## Function Documentation

## ◆ ili9341_rotateOutput()

void ili9341_rotateOutput | ( | uint8_t | on | ) |

Sets rotation of all output functions.

Sets rotation of all output functions. 0 - no rotation, 1 - change by 90 degrees Actually doesn't change screen orientation, only rotates primitives being output

Parameters

  on | enable (1) of disable (0)

Warning
  experimental feature, may work incorrectly

Definition at line 279 of file lcd_ili9341.c.

## ◆ ili9341_setRotation()

void ili9341_setRotation | ( | uint8_t | rotation | ) |

Sets screen orientation (rotation)

Sets screen orientation (rotation): 0 - normal, 1 - 90 CW, 2 - 180 CW, 3 - 270 CW

Parameters

  rotation | - screen rotation 0 - normal, 1 - 90 CW, 2 - 180 CW, 3 - 270 CW

Note
  works only with ili9341 display

Definition at line 231 of file lcd_ili9341.c.