SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

vga_monitor.h
Go to the documentation of this file.
1 /*
2 MIT License
3
4 Copyright (c) 2018, Alexey Dynda
5
6 Permission is hereby granted, free of charge, to any person obtaining a copy
7 of this software and associated documentation files (the "Software"), to deal
8 in the Software without restriction, including without limitation the rights
9 to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
10 copies of the Software, and to permit persons to whom the Software is
11 furnished to do so, subject to the following conditions:
12
13 The above copyright notice and this permission notice shall be included in all
14 copies or substantial portions of the Software.
15
16 THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
17 IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
18 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
19 AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
20 LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
21 OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
22 SOFTWARE.
23 */
28 #ifndef _SSD1306_VGA_MONITOR_H_
29 #define _SSD1306_VGA_MONITOR_H_
30
31 #include "ssd1306_hal/io.h"
32
33 #ifdef __cplusplus
34 extern "C" {
35 #endif
36
52 void vga_96x40_8colors_init(void);
53
64 void vga_128x64_mono_init(void);
65
70 #ifdef __cplusplus
71 }
72 #endif
73
74 #endif
75
io.h
vga_128x64_mono_init
void vga_128x64_mono_init(void)
Inits 128x64 monochrome VGA display.
Definition: vga_monitor.c:134
vga_96x40_8colors_init
void vga_96x40_8colors_init(void)
Inits 96x40 color VGA display.
Definition: vga_monitor.c:121