SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Public Member Functions | Public Attributes | Static Public Attributes | Protected Attributes | List of all members
AdafruitCanvasOps< BPP > Class Template Reference
NANO_ENGINE: Nano Engine description

`#include <adafruit.h>`

Inheritance diagram for AdafruitCanvasOps< BPP >:

## Public Member Functions
| AdafruitCanvasOps (lcduint_t w, lcduint_t h, uint8_t *buffer)
void | drawPixel (int16_t x, int16_t y, uint16_t color) override
void | setOffset (lcdint_t ox, lcdint_t oy)

## Public Attributes
NanoPoint | offset

## Static Public Attributes
static const uint8_t | BITS_PER_PIXEL = BPP

## Protected Attributes
uint8_t * | m_buffer

## Detailed Description

### template<uint8_t BPP>
class AdafruitCanvasOps< BPP >

This is basic template class for all canvas classes, based on Adafruit_GFX. This base class provides functionality compatible with native NanoCanvas implementation of ssd1306 library

Definition at line 71 of file adafruit.h.

## Constructor & Destructor Documentation

## ◆ AdafruitCanvasOps()

template<uint8_t BPP>

AdafruitCanvasOps< BPP >::AdafruitCanvasOps | ( | lcduint_t | w,
|  | lcduint_t | h,
|  | uint8_t * | buffer
| ) |  |
| inline

Initializes canvas, based on Adafruit GFX.

Parameters

  w | width of canvas
  h | height of canvas area
  buffer | buffer to use for pixels

Note
  the size of buffer must be enough to store (w*h*bpp/8) bytes.

Definition at line 88 of file adafruit.h.

## Member Function Documentation

## ◆ drawPixel()

template<uint8_t BPP>

void AdafruitCanvasOps< BPP >::drawPixel | ( | int16_t | x,
|  | int16_t | y,
|  | uint16_t | color
| ) |  |
| override

draw single pixel in canvas area

Parameters

  x | x position
  y | y position
  color | color of pixel: for monochrome it can be 0 (black), 1 (white), 2 (invert)

## ◆ setOffset()

template<uint8_t BPP>

void AdafruitCanvasOps< BPP >::setOffset | ( | lcdint_t | ox,
|  | lcdint_t | oy
| ) |  |
| inline

Sets offset

Parameters

  ox | - X offset in pixels
  oy | - Y offset in pixels

Definition at line 110 of file adafruit.h.

## Member Data Documentation

## ◆ BITS_PER_PIXEL

template<uint8_t BPP>

const uint8_t AdafruitCanvasOps< BPP >::BITS_PER_PIXEL = BPP
| static

number of bits per single pixel in buffer

Definition at line 78 of file adafruit.h.

## ◆ m_buffer

template<uint8_t BPP>

uint8_t* AdafruitCanvasOps< BPP >::m_buffer
| protected

pixels buffer

Definition at line 110 of file adafruit.h.

## ◆ offset

template<uint8_t BPP>

NanoPoint AdafruitCanvasOps< BPP >::offset

Fixed offset for all operation of NanoCanvasOps in pixels.

Definition at line 75 of file adafruit.h.

The documentation for this class was generated from the following file:

- nano_engine/adafruit.h