SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

platform.c
1 /*
2 MIT License
3
4 Copyright (c) 2018, Alexey Dynda
5
6 Permission is hereby granted, free of charge, to any person obtaining a copy
7 of this software and associated documentation files (the "Software"), to deal
8 in the Software without restriction, including without limitation the rights
9 to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
10 copies of the Software, and to permit persons to whom the Software is
11 furnished to do so, subject to the following conditions:
12
13 The above copyright notice and this permission notice shall be included in all
14 copies or substantial portions of the Software.
15
16 THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
17 IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
18 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
19 AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
20 LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
21 OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
22 SOFTWARE.
23 */
24
25 #if defined(__MINGW32__)
26
27 #include "ssd1306_hal/io.h"
28
29 #include "intf/ssd1306_interface.h"
30 #include "intf/i2c/ssd1306_i2c.h"
31 #include "intf/ssd1306_interface.h"
32 #include "intf/spi/ssd1306_spi_conf.h"
33 #include "intf/spi/ssd1306_spi.h"
34
35 #include <stdio.h>
36 #include <unistd.h>
37
38 #if !defined(SDL_EMULATION)
39
40 #include <errno.h>
41 #include <fcntl.h>
42 #include <sys/ioctl.h>
43 #include <linux/i2c-dev.h>
44 #include <stdlib.h>
45 #include <linux/spi/spidev.h>
46
47 #endif
48
50 // MINGW I2C IMPLEMENTATION
52 #if defined(CONFIG_PLATFORM_I2C_AVAILABLE) && defined(CONFIG_PLATFORM_I2C_ENABLE)
53
54 #if !defined(SDL_EMULATION)
55
56 static uint8_t s_sa = SSD1306_SA;
57 static int s_fd = -1;
58 static uint8_t s_buffer[128];
59 static uint8_t s_dataSize = 0;
60
61 static void platform_i2c_start(void)
62 {
63 s_dataSize = 0;
64 }
65
66 static void platform_i2c_stop(void)
67 {
68 if (write(s_fd, s_buffer, s_dataSize) != s_dataSize)
69 {
70 fprintf(stderr, "Failed to write to the i2c bus: %s.\n", strerror(errno));
71 }
72 s_dataSize = 0;
73 }
74
75 static void platform_i2c_send(uint8_t data)
76 {
77 s_buffer[s_dataSize] = data;
78 s_dataSize++;
79 if (s_dataSize == sizeof(s_buffer))
80 {
81 /* Send function puts all data to internal buffer. *
82 * Restart transmission if internal buffer is full. */
83 ssd1306_intf.stop();
84 ssd1306_intf.start();
85 ssd1306_intf.send(0x40);
86 }
87 }
88
89 static void platform_i2c_send_buffer(const uint8_t *buffer, uint16_t size)
90 {
91 while (size--)
92 {
93 platform_i2c_send(*buffer);
94 buffer++;
95 }
96 }
97
98 static void platform_i2c_close()
99 {
100 if (s_fd >= 0)
101 {
102 close(s_fd);
103 s_fd = -1;
104 }
105 }
106
107 static void empty_function()
108 {
109 }
110
111 static void empty_function_single_arg(uint8_t arg)
112 {
113 }
114
115 static void empty_function_two_args(const uint8_t *arg1, uint16_t arg2)
116 {
117 }
118
119 void ssd1306_platform_i2cInit(int8_t busId, uint8_t sa, ssd1306_platform_i2cConfig_t * cfg)
120 {
121 char filename[20];
122 if (busId < 0)
123 {
124 busId = 1;
125 }
126 snprintf(filename, 19, "/dev/i2c-%d", busId);
127 ssd1306_intf.start = empty_function;
128 ssd1306_intf.stop = empty_function;
129 ssd1306_intf.close = empty_function;
130 ssd1306_intf.send = empty_function_single_arg;
131 ssd1306_intf.send_buffer = empty_function_two_args;
132 if ((s_fd = open(filename, O_RDWR)) < 0)
133 {
134 fprintf(stderr, "Failed to open the i2c bus\n");
135 return;
136 }
137 if (sa)
138 {
139 s_sa = sa;
140 }
141 if (ioctl(s_fd, I2C_SLAVE, s_sa) < 0)
142 {
143 fprintf(stderr, "Failed to acquire bus access and/or talk to slave.\n");
144 return;
145 }
146 ssd1306_intf.start = platform_i2c_start;
147 ssd1306_intf.stop = platform_i2c_stop;
148 ssd1306_intf.send = platform_i2c_send;
149 ssd1306_intf.send_buffer = platform_i2c_send_buffer;
150 ssd1306_intf.close = platform_i2c_close;
151 }
152
153 #else /* SDL_EMULATION */
154
155 #include "sdl_core.h"
156
157 static void platform_i2c_send_buffer(const uint8_t *buffer, uint16_t size)
158 {
159 while (size--)
160 {
161 sdl_send_byte(*buffer);
162 buffer++;
163 };
164 }
165
166 void ssd1306_platform_i2cInit(int8_t busId, uint8_t sa, ssd1306_platform_i2cConfig_t * cfg)
167 {
168 sdl_core_init();
169 ssd1306_intf.spi = 0;
170 ssd1306_intf.start = sdl_send_init;
171 ssd1306_intf.stop = sdl_send_stop;
172 ssd1306_intf.send = sdl_send_byte;
173 ssd1306_intf.send_buffer = platform_i2c_send_buffer;
174 ssd1306_intf.close = sdl_core_close;
175 }
176
177 #endif /* SDL_EMULATION */
178
179 #endif // CONFIG_PLATFORM_I2C_AVAILABLE
180
181
183 // MINGW SPI IMPLEMENTATION
185 #if defined(CONFIG_PLATFORM_SPI_AVAILABLE) && defined(CONFIG_PLATFORM_SPI_ENABLE)
186
187 #if !defined(SDL_EMULATION)
188
189 static int s_spi_fd = -1;
190 extern uint32_t s_ssd1306_spi_clock;
191
192 static void platform_spi_start(void)
193 {
194 }
195
196 static void platform_spi_stop(void)
197 {
198 }
199
200 static void platform_spi_send(uint8_t data)
201 {
202 /* TODO: Yeah, sending single bytes is too slow, but *
203 * need to figure out how to detect data/command bytes *
204 * to send bytes as one block */
205 uint8_t buf[1];
206 struct spi_ioc_transfer mesg;
207 buf[0] = data;
208 memset(&mesg, 0, sizeof mesg);
209 mesg.tx_buf = (unsigned long)&buf[0];
210 mesg.rx_buf = 0;
211 mesg.len = 1;
212 mesg.delay_usecs = 0;
213 mesg.speed_hz = 0;
214 mesg.bits_per_word = 8;
215 mesg.cs_change = 0;
216 if (ioctl(s_spi_fd, SPI_IOC_MESSAGE(1), &mesg) < 1)
217 {
218 fprintf(stderr, "SPI failed to send SPI message: %s\n", strerror (errno)) ;
219 }
220 }
221
222 static void platform_spi_close(void)
223 {
224 if (s_spi_fd >= 0)
225 {
226 close(s_spi_fd);
227 s_spi_fd = -1;
228 }
229 }
230
231 static void platform_spi_send_buffer(const uint8_t *data, uint16_t len)
232 {
233 while (len--)
234 {
235 platform_spi_send(*data);
236 data++;
237 }
238 }
239
240 static void empty_function_spi(void)
241 {
242 }
243
244 static void empty_function_arg_spi(uint8_t byte)
245 {
246 }
247
248 static void empty_function_args_spi(const uint8_t *buffer, uint16_t bytes)
249 {
250 }
251
252 void ssd1306_platform_spiInit(int8_t busId,
253 int8_t ces,
254 int8_t dcPin)
255 {
256 char filename[20];
257 if (busId < 0)
258 {
259 busId = 0;
260 }
261 if (ces < 0)
262 {
263 ces = 0;
264 }
265 s_ssd1306_cs = -1; // SPI interface does't need separate ces pin
266 s_ssd1306_dc = dcPin;
267 ssd1306_intf.spi = 1;
268 ssd1306_intf.start = empty_function_spi;
269 ssd1306_intf.stop = empty_function_spi;
270 ssd1306_intf.send = empty_function_arg_spi;
271 ssd1306_intf.send_buffer = empty_function_args_spi;
272 ssd1306_intf.close = empty_function;
273
274 snprintf(filename, 19, "/dev/spidev%d.%d", busId, ces);
275 if ((s_spi_fd = open(filename, O_RDWR)) < 0)
276 {
277 printf("Failed to initialize SPI: %s!\n", strerror(errno));
278 return;
279 }
280 unsigned int speed = s_ssd1306_spi_clock;
281 if (ioctl(s_spi_fd, SPI_IOC_WR_MAX_SPEED_HZ, &speed) < 0)
282 {
283 printf("Failed to set speed on SPI line: %s!\n", strerror(errno));
284 }
285 uint8_t mode = SPI_MODE_0;
286 if (ioctl (s_spi_fd, SPI_IOC_WR_MODE, &mode) < 0)
287 {
288 printf("Failed to set SPI mode: %s!\n", strerror(errno));
289 }
290 uint8_t spi_bpw = 8;
291 if (ioctl (s_spi_fd, SPI_IOC_WR_BITS_PER_WORD, &spi_bpw) < 0)
292 {
293 printf("Failed to set SPI BPW: %s!\n", strerror(errno));
294 }
295
296 ssd1306_intf.spi = 1;
297 ssd1306_intf.start = platform_spi_start;
298 ssd1306_intf.stop = platform_spi_stop;
299 ssd1306_intf.send = platform_spi_send;
300 ssd1306_intf.send_buffer = platform_spi_send_buffer;
301 ssd1306_intf.close = platform_spi_close;
302 }
303
304 #else /* SDL_EMULATION */
305
306 #include "sdl_core.h"
307
308 static void sdl_send_bytes(const uint8_t *buffer, uint16_t size)
309 {
310 while (size--)
311 {
312 sdl_send_byte(*buffer);
313 buffer++;
314 };
315 }
316
317 void ssd1306_platform_spiInit(int8_t busId, int8_t ces, int8_t dcPin)
318 {
319 sdl_core_init();
320 if (ces >= 0)
321 {
322 s_ssd1306_cs = ces;
323 }
324 if (dcPin >= 0)
325 {
326 s_ssd1306_dc = dcPin;
327 }
328 sdl_set_dc_pin(dcPin);
329 ssd1306_intf.spi = 1;
330 ssd1306_intf.start = sdl_send_init;
331 ssd1306_intf.stop = sdl_send_stop;
332 ssd1306_intf.send = sdl_send_byte;
333 ssd1306_intf.send_buffer = sdl_send_bytes;
334 ssd1306_intf.close = sdl_core_close;
335 }
336
337 #endif /* SDL_EMULATION */
338
339 #endif // CONFIG_PLATFORM_SPI_AVAILABLE
340
341 #endif // __MINGW32__
342
s_ssd1306_dc
int8_t s_ssd1306_dc
Definition: ssd1306_spi.c:34
ssd1306_platform_i2cConfig_t
Definition: io.h:80
ssd1306_platform_spiInit
void ssd1306_platform_spiInit(int8_t busId, int8_t cesPin, int8_t dcPin)
Initializes spi interface for platform being used.
ssd1306_interface_t::send
void(* send)(uint8_t data)
Definition: ssd1306_interface.h:70
ssd1306_interface_t::stop
void(* stop)(void)
Definition: ssd1306_interface.h:65
s_ssd1306_spi_clock
uint32_t s_ssd1306_spi_clock
Definition: ssd1306_spi.c:35
io.h
ssd1306_i2c.h
ssd1306_platform_i2cInit
void ssd1306_platform_i2cInit(int8_t busId, uint8_t addr, ssd1306_platform_i2cConfig_t *cfg)
Initializes i2c interface for platform being used.
ssd1306_spi_conf.h
ssd1306_spi.h
ssd1306_interface_t::start
void(* start)(void)
Definition: ssd1306_interface.h:61
ssd1306_interface_t::close
void(* close)(void)
deinitializes internal resources, allocated for interface.
Definition: ssd1306_interface.h:88
ssd1306_intf
ssd1306_interface_t ssd1306_intf
Definition: ssd1306_interface.c:31
SSD1306_SA
#define SSD1306_SA
Definition: ssd1306_i2c_conf.h:47
ssd1306_interface.h
ssd1306_interface_t::spi
uint8_t spi
Definition: ssd1306_interface.h:57
ssd1306_interface_t::send_buffer
void(* send_buffer)(const uint8_t *buffer, uint16_t size)
Sends bytes to SSD1306 device.
Definition: ssd1306_interface.h:80
s_ssd1306_cs
int8_t s_ssd1306_cs
Definition: ssd1306_spi.c:33