SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Classes | Macros | Enumerations | Functions | Variables
lcd_common.h File Reference
`#include "ssd1306_hal/io.h"`

Go to the source code of this file.

## Classes
struct | ssd1306_lcd_t

## Macros
#define | s_displayHeight ssd1306_lcd.height
#define | s_displayWidth ssd1306_lcd.width
#define | g_lcd_type ssd1306_lcd.type
#define | ssd1306_setRamBlock ssd1306_lcd.set_block
| Sets block in RAM of lcd display controller to write data to. More...
#define | ssd1306_nextRamPage ssd1306_lcd.next_page
#define | ssd1306_sendPixels ssd1306_lcd.send_pixels1
#define | ssd1306_sendPixelsBuffer ssd1306_lcd.send_pixels_buffer1
#define | ssd1306_sendPixel8 ssd1306_lcd.send_pixels8
| Sends RGB pixel encoded in 3-3-2 format to OLED driver. Sends RGB pixel encoded in 3-3-2 format to OLED driver. More...
#define | SSD1306_COMPAT_SPI_BLOCK_8BIT_CMDS(column_cmd, row_cmd)
#define | CONTROLLER_NATIVE_SPI_BLOCK_8BIT_CMDS(column_cmd, row_cmd)
#define | SSD1306_COMPAT_SEND_PIXELS_RGB8_CMDS()
#define | SSD1306_COMPAT_SEND_PIXELS_RGB16_CMDS()

## Enumerations
enum | lcd_type_t { LCD_TYPE_SSD1306, LCD_TYPE_PCD8544, LCD_TYPE_SH1106, LCD_TYPE_SSD1331, LCD_TYPE_CUSTOM }
enum | lcd_mode_t { LCD_MODE_NORMAL = 0, LCD_MODE_SSD1306_COMPAT = 1 }

## Functions
void | ssd1306_sendData (uint8_t data) __attribute__((deprecated))
void | ssd1306_configureI2cDisplay (const uint8_t *config, uint8_t configSize)
| Sends configuration being passed to lcd display i2c/spi controller. More...
void | ssd1306_configureSpiDisplay (const uint8_t *config, uint8_t configSize)
| Sends configuration being passed to lcd display spi controller. More...
void | ssd1306_configureSpiDisplay2 (const uint8_t *config, uint8_t configSize)
| Sends configuration being passed to lcd display spi controller. More...
void | ssd1306_setMode (lcd_mode_t mode)
| Sets library display mode for direct draw functions. More...
void | ssd1306_resetController (int8_t rstPin, uint8_t delayMs)
| Does hardware reset for oled controller. More...

## Variables
ssd1306_lcd_t | ssd1306_lcd

## Detailed Description

global lcd settings

Definition in file lcd_common.h.