SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

lcd_il9163.h
Go to the documentation of this file.
1 /*
2 MIT License
3
4 Copyright (c) 2018-2020, Alexey Dynda
5
6 Permission is hereby granted, free of charge, to any person obtaining a copy
7 of this software and associated documentation files (the "Software"), to deal
8 in the Software without restriction, including without limitation the rights
9 to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
10 copies of the Software, and to permit persons to whom the Software is
11 furnished to do so, subject to the following conditions:
12
13 The above copyright notice and this permission notice shall be included in all
14 copies or substantial portions of the Software.
15
16 THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
17 IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
18 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
19 AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
20 LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
21 OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
22 SOFTWARE.
23 */
29 #ifndef _TFT_IL9163_H_
30 #define _TFT_IL9163_H_
31
32 #include "ssd1306_hal/io.h"
33 #include "lcd/lcd_common.h"
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
57 void il9163_setMode(lcd_mode_t mode);
58
67 void il9163_128x128_init(void);
68
76 void il9163_setOffset(lcdint_t x, lcdint_t y);
77
86 void st7735_128x160_init(void);
87
96 void il9163_128x128_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin);
97
106 void st7735_128x160_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin);
107
124 void il9163_setRotation(uint8_t rotation);
125
133 #define st7735_setRotation il9163_setRotation
134
139 #ifdef __cplusplus
140 }
141 #endif
142
143 // ----------------------------------------------------------------------------
144 #endif // _TFT_IL9163_H_
st7735_128x160_init
void st7735_128x160_init(void)
Inits 128x160 RGB OLED display (based on st7735 controller).
Definition: lcd_il9163.c:406
st7735_128x160_spi_init
void st7735_128x160_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin)
Inits 128x160 RGB TFT display over spi (based on st7735 controller).
Definition: lcd_il9163.c:422
lcd_common.h
io.h
lcd_mode_t
lcd_mode_t
Definition: lcd_common.h:69
il9163_setRotation
void il9163_setRotation(uint8_t rotation)
Sets screen orientation (rotation)
Definition: lcd_il9163.c:288
il9163_128x128_init
void il9163_128x128_init(void)
Inits 128x128 RGB OLED display (based on il9163 controller).
Definition: lcd_il9163.c:253
il9163_setOffset
void il9163_setOffset(lcdint_t x, lcdint_t y)
Sets screen offset (refer to datasheet of your display)
Definition: lcd_il9163.c:176
il9163_128x128_spi_init
void il9163_128x128_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin)
Inits 128x128 RGB TFT display over spi (based on il9163 controller).
Definition: lcd_il9163.c:269
il9163_setMode
void il9163_setMode(lcd_mode_t mode)
Sets GDRAM autoincrement mode.
Definition: lcd_il9163.c:192