SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Functions
SSD1331: ssd1331 control functions

## Functions
void | ssd1331_setRotation (uint8_t rotation)
| Sets screen orientation (rotation) More...

## Detailed Description

## Function Documentation

## ◆ ssd1331_setRotation()

void ssd1331_setRotation | ( | uint8_t | rotation | ) |

Sets screen orientation (rotation)

Sets screen orientation (rotation): 0 - normal, 1 - 90 CW, 2 - 180 CW, 3 - 270 CW

Parameters

  rotation | - screen rotation 0 - normal, 1 - 90 CW, 2 - 180 CW, 3 - 270 CW

Note
  works only with ssd1331 display

Definition at line 130 of file oled_ssd1331.c.