SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

lcd_ili9341.h
Go to the documentation of this file.
1 /*
2 MIT License
3
4 Copyright (c) 2018, Alexey Dynda
5
6 Permission is hereby granted, free of charge, to any person obtaining a copy
7 of this software and associated documentation files (the "Software"), to deal
8 in the Software without restriction, including without limitation the rights
9 to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
10 copies of the Software, and to permit persons to whom the Software is
11 furnished to do so, subject to the following conditions:
12
13 The above copyright notice and this permission notice shall be included in all
14 copies or substantial portions of the Software.
15
16 THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
17 IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
18 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
19 AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
20 LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
21 OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
22 SOFTWARE.
23 */
29 #ifndef _TFT_ILI9341_H_
30 #define _TFT_ILI9341_H_
31
32 #include "ssd1306_hal/io.h"
33 #include "lcd/lcd_common.h"
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
57 void ili9341_setMode(lcd_mode_t mode);
58
67 void ili9341_240x320_init(void);
68
77 void ili9341_240x320_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin);
78
95 void ili9341_setRotation(uint8_t rotation);
96
106 void ili9341_rotateOutput(uint8_t on);
107
112 #ifdef __cplusplus
113 }
114 #endif
115
116 // ----------------------------------------------------------------------------
117 #endif // _TFT_ILI9141_H_
lcd_common.h
ili9341_setRotation
void ili9341_setRotation(uint8_t rotation)
Sets screen orientation (rotation)
Definition: lcd_ili9341.c:231
ili9341_240x320_spi_init
void ili9341_240x320_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin)
Inits 240x320 RGB TFT display over spi (based on ili9341 controller).
Definition: lcd_ili9341.c:212
io.h
ili9341_240x320_init
void ili9341_240x320_init(void)
Inits 240x320 RGB OLED display (based on ili9341 controller).
Definition: lcd_ili9341.c:196
lcd_mode_t
lcd_mode_t
Definition: lcd_common.h:69
ili9341_setMode
void ili9341_setMode(lcd_mode_t mode)
Sets GDRAM autoincrement mode.
Definition: lcd_ili9341.c:139
ili9341_rotateOutput
void ili9341_rotateOutput(uint8_t on)
Sets rotation of all output functions.
Definition: lcd_ili9341.c:279