# RT

Aim to demonstrate Real Time capabilities of the OS.

- Use of Arduino Mega 2560 at 16MHz
- Use a logic analyser to measure timings.
  - Acquisition frequency: 100Hz

Thread switch is 10.75µs, in other words

![](./avrtos_thread_switch_duration.png)