# TCN75 I2C Temperature Sensor

Following capture show the I2C communication between the AVR and the TCN75 temperature sensor using the `i2c_master_write_read()` function.

![i2c-write-read.png](i2c-write-read.png)