# SPI Master

For my test the master is an Arduino Ethernet.

## Send interval

You can tune the send interval by tuning the `DELAY_US` macro.

We can't precily configure the data rate, but it's convenient for testing.
