================
Supported Boards
================

.. list-table::

   * - Board Name
     - CPU
     - Memory
     - Display
     - `Board <https://lvgl.io/boards>`__ video
     - Links
   * - **EK-RA8D1**
     -
         | 480 MHz
         | Arm Cortex-M85
     -
         | 1MB internal SDRAM
         | 64MB external SDRAM
         | 2MB internal flash
         | 64MB external octo-SPI flash
     -
         | 4.5”
         | 480x854
         | 2-lane MIPI
     - .. raw:: html

           <iframe width="320" height="180" src="https://www.youtube.com/embed/WkJPB8wto_U" title="YouTube video player" frameborder="0" allow="accelerometer; autoplay; clipboard-write; encrypted-media; gyroscope; picture-in-picture; web-share" referrerpolicy="strict-origin-when-cross-origin" allowfullscreen></iframe>

     - `Demo repository <https://github.com/lvgl/lv_port_renesas_ek-ra8d1>`__
   * - **EK-RA8P1**
     -
         | 1 GHz
         | Arm Cortex-M85
     -
         | 1872KB internal
         | 128MB external
         | 1MB internal flash
     -
         | 7”
         | 1024x600
         | Parallel RGB888
     - .. raw:: html

           <iframe width="320" height="180" src="https://www.youtube.com/embed/PoxDoQp51G8" title="YouTube video player" frameborder="0" allow="accelerometer; autoplay; clipboard-write; encrypted-media; gyroscope; picture-in-picture; web-share" referrerpolicy="strict-origin-when-cross-origin" allowfullscreen></iframe>

     - `Demo repository <https://github.com/lvgl/lv_port_renesas_ek_ra8p1>`__
   * - **EK-RA6M3G**
     -
         | 120 MHz
         | Arm Cortex-M4
     -
         | 640kB internal SRAM
         | 2MB internal SRAM
         | 32MB external QSPI flash
     -
         | 4.3”
         | 480x272
         | Parallel RGB565
     - .. raw:: html

           <iframe width="320" height="180" src="https://www.youtube.com/embed/0kar4Ee3Qic" title="YouTube video player" frameborder="0" allow="accelerometer; autoplay; clipboard-write; encrypted-media; gyroscope; picture-in-picture; web-share" referrerpolicy="strict-origin-when-cross-origin" allowfullscreen></iframe>

     -
         | `Demo repository <https://github.com/lvgl/lv_port_renesas_ek-ra6m3g>`__
   * - **RX72N Envision Kit**
     -
         | 240 MHz
         | Renesas RXv3
     -
         | 1MB internal SRAM
         | 4MB internal SRAM
         | 32MB external QSPI flash
     -
         | 4.3”
         | 480x272
         | Parallel RGB565
     - .. raw:: html

           <iframe width="320" height="180" src="https://www.youtube.com/embed/__56v8DsfH0" title="YouTube video player" frameborder="0" allow="accelerometer; autoplay; clipboard-write; encrypted-media; gyroscope; picture-in-picture; web-share" referrerpolicy="strict-origin-when-cross-origin" allowfullscreen></iframe>

     - `Demo repository <https://github.com/lvgl/lv_port_renesas_rx72n-envision-kit>`__
   * - **RZ/G2L-EVKIT**
     -
         | 1.2 GHz
         | Arm Cortex-A55
     -
         | 2GB DDR4 SDRAM
     -
         | 1920x1080
         | Micro-HDMI
     - .. raw:: html

           <iframe width="320" height="180" src="https://www.youtube.com/embed/oeuVvB7y-QA" title="YouTube video player" frameborder="0" allow="accelerometer; autoplay; clipboard-write; encrypted-media; gyroscope; picture-in-picture; web-share" referrerpolicy="strict-origin-when-cross-origin" allowfullscreen></iframe>

     - `Demo repository <https://github.com/lvgl/lv_port_renesas_rz-g2l-evkit>`__
   * - **RZ/G2UL-EVKIT**
     -
         | 1.0 GHz
         | Arm Cortex-A55
     -
         | 1GB DDR4 SDRAM
     -
         | 1280x800
         | Parallel RGB888
         | with Micro-HDMI bridge
     - .. raw:: html

           <iframe width="320" height="180" src="https://www.youtube.com/embed/VnynDLR36Xc" title="YouTube video player" frameborder="0" allow="accelerometer; autoplay; clipboard-write; encrypted-media; gyroscope; picture-in-picture; web-share" referrerpolicy="strict-origin-when-cross-origin" allowfullscreen></iframe>

     - `Demo repository <https://github.com/lvgl/lv_port_renesas_rz-g2ul-evkit>`__
   * - **RZ/A3M**
     -
         | 1.0 GHz
         | Arm Cortex-A55
     -
         | 128MB internal DDR3L-SDRAM
         | 128KB internal SRAM
         | 128MB external QSPI NAND flash
         | 32MB external QSPI NOR flash
     -
         | 4.3”
         | 1280x720
         | MIPI
     - .. raw:: html

           <iframe width="320" height="180" src="https://www.youtube.com/embed/IEjBGgrR_mk" title="YouTube video player" frameborder="0" allow="accelerometer; autoplay; clipboard-write; encrypted-media; gyroscope; picture-in-picture; web-share" referrerpolicy="strict-origin-when-cross-origin" allowfullscreen></iframe>

     - `Demo repository <https://github.com/lvgl/lv_port_renesas-ek-rz_a3m>`__
