# nodeMCU-SoilMoisture_ST-8563

This repository contains the Arduino script to connect a Soil-Moisture sensor ().
The sensor is connecting and sending data to t6 only during daylight: using a RTC clock ST-8563.

## Installation

Just clone the repository and upload the .ino file onto your Arduino board.

## Contributors

Mathieu L. <mathieu@internetcollaboratif.info>

## License

[GNU General Public License v3.0](https://www.gnu.org/licenses/gpl-3.0.html)
