MycilaJSY 13.0.0 Arduino / ESP32 library for the JSY1031, JSY-MK-163, JSY-MK-193, JSY-MK-194, JSY-MK-227, JSY-MK-229, JSY-MK-333 families single-phase and three-phase AC bidirectional meters from Shenzhen Jiansiyan Technologies Co, Ltd.

Loading...
Searching...
No Matches
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - a -

- activeEnergy : Mycila::JSY::Metrics
- activeEnergyImported : Mycila::JSY::Metrics
- activeEnergyReturned : Mycila::JSY::Metrics
- activePower : Mycila::JSY::Metrics
- apparentEnergy : Mycila::JSY::Metrics
- apparentPower : Mycila::JSY::Metrics

### - b -

- begin() : Mycila::JSY

### - c -

- current : Mycila::JSY::Metrics

### - d -

- dimmedVoltage() : Mycila::JSY::Metrics

### - e -

- end() : Mycila::JSY

### - f -

- frequency : Mycila::JSY::Metrics

### - g -

- getDestinationAddress() : Mycila::JSY
- getLastAddress() : Mycila::JSY
- getMaxAvailableBaudRate() : Mycila::JSY
- getModel() : Mycila::JSY
- getModelName() : Mycila::JSY
- getTime() : Mycila::JSY

### - i -

- isBaudRateSupported() : Mycila::JSY

### - n -

- nominalPower() : Mycila::JSY::Metrics

### - p -

- phaseAngleI : Mycila::JSY::Metrics
- phaseAngleU : Mycila::JSY::Metrics
- phaseAngleUI : Mycila::JSY::Metrics
- powerFactor : Mycila::JSY::Metrics

### - r -

- reactiveEnergy : Mycila::JSY::Metrics
- reactiveEnergyImported : Mycila::JSY::Metrics
- reactiveEnergyReturned : Mycila::JSY::Metrics
- reactivePower : Mycila::JSY::Metrics
- read() : Mycila::JSY
- readMode() : Mycila::JSY
- readModel() : Mycila::JSY
- resetEnergy() : Mycila::JSY
- resistance() : Mycila::JSY::Metrics

### - s -

- setBaudRate() : Mycila::JSY
- setDeviceAddress() : Mycila::JSY
- setMode() : Mycila::JSY

### - t -

- thdI : Mycila::JSY::Metrics
- thdi() : Mycila::JSY::Metrics
- thdU : Mycila::JSY::Metrics

### - v -

- voltage : Mycila::JSY::Metrics