MycilaJSY 13.0.0 Arduino / ESP32 library for the JSY1031, JSY-MK-163, JSY-MK-193, JSY-MK-194, JSY-MK-227, JSY-MK-229, JSY-MK-333 families single-phase and three-phase AC bidirectional meters from Shenzhen Jiansiyan Technologies Co, Ltd.

Loading...
Searching...
No Matches
Here is a list of all documented functions with links to the struct/union documentation for each field:

- begin() : Mycila::JSY
- dimmedVoltage() : Mycila::JSY::Metrics
- end() : Mycila::JSY
- getDestinationAddress() : Mycila::JSY
- getLastAddress() : Mycila::JSY
- getMaxAvailableBaudRate() : Mycila::JSY
- getModel() : Mycila::JSY
- getModelName() : Mycila::JSY
- getTime() : Mycila::JSY
- isBaudRateSupported() : Mycila::JSY
- nominalPower() : Mycila::JSY::Metrics
- read() : Mycila::JSY
- readMode() : Mycila::JSY
- readModel() : Mycila::JSY
- resetEnergy() : Mycila::JSY
- resistance() : Mycila::JSY::Metrics
- setBaudRate() : Mycila::JSY
- setDeviceAddress() : Mycila::JSY
- setMode() : Mycila::JSY
- thdi() : Mycila::JSY::Metrics