MakeBlock Drive Updated Updated library for MakeBlock Ranger

Loading...
Searching...
No Matches
MeEncoderNew Member List

This is the complete list of members for MeEncoderNew, including all inherited members.

begin(void) | MeEncoderNew |
getCurrentPosition(void) | MeEncoderNew |
getCurrentSpeed(void) | MeEncoderNew |
getFirmwareVersion(char *buffer) | MeEncoderNew |
getPosPID(float *p, float *i, float *d) | MeEncoderNew |
getPulse(void) | MeEncoderNew |
getRatio(void) | MeEncoderNew |
getSpeedPID(float *p, float *i, float *d) | MeEncoderNew |
isTarPosReached(void) | MeEncoderNew |
MeEncoderNew(uint8_t addr, uint8_t slot) | MeEncoderNew |
MeEncoderNew(uint8_t slot) | MeEncoderNew |
MeEncoderNew(void) | MeEncoderNew |
move(long angle, float speed=220, float lock_state=1) | MeEncoderNew |
moveTo(long angle, float speed=220, float lock_state=1) | MeEncoderNew |
reset(void) | MeEncoderNew |
runSpeed(float speed, float lock_state=1) | MeEncoderNew |
runSpeedAndTime(float speed, float time, float lock_state=1) | MeEncoderNew |
runTurns(long turns, float speed=220, float lock_state=1) | MeEncoderNew |
setAddr(uint8_t i2cAddr, uint8_t slot) | MeEncoderNew |
setCurrentPosition(long pulse_counter) | MeEncoderNew |
setDevid(uint8_t devid) | MeEncoderNew |
setMode(uint8_t mode) | MeEncoderNew |
setPosPID(float p, float i, float d) | MeEncoderNew |
setPulse(int p) | MeEncoderNew |
setPWM(int pwm) | MeEncoderNew |
setRatio(float r) | MeEncoderNew |
setSpeedPID(float p, float i, float d) | MeEncoderNew |