MakeBlock Drive Updated Updated library for MakeBlock Ranger

Loading...
Searching...
No Matches
MeSmartServo Member List

This is the complete list of members for MeSmartServo, including all inherited members.

_bitPeriod (defined in MeSerial) | MeSerial | protected
_byte (defined in MeSerial) | MeSerial | protected
_hard (defined in MeSerial) | MeSerial | protected
_lastTime (defined in MeSerial) | MeSerial | protected
_polling (defined in MeSerial) | MeSerial | protected
_port | MePort | protected
_scratch (defined in MeSerial) | MeSerial | protected
_slot | MePort | protected
aRead1(void) | MePort |
aRead2(void) | MePort |
assignDevIdRequest(void) | MeSmartServo |
assignDevIdResponse(void *arg) | MeSmartServo |
available() | MeSerial | virtual
aWrite1(int16_t value) | MePort |
aWrite2(int16_t value) | MePort |
begin(long baudrate) | MeSerial |
buffer (defined in MeSerial) | MeSerial | protected
bufferIndex (defined in MeSerial) | MeSerial | protected
concatenateWith(String s1, String s2) (defined in MeSerial) | MeSerial |
dataLineAvailable(void) (defined in MeSerial) | MeSerial |
dpRead1(void) | MePort |
dpRead2(void) | MePort |
dRead1(uint8_t mode=INPUT) | MePort |
dRead2(uint8_t mode=INPUT) | MePort |
dWrite1(bool value) | MePort |
dWrite2(bool value) | MePort |
end(void) | MeSerial |
equalString(String s1, String s2) (defined in MeSerial) | MeSerial |
errorCodeCheckResponse(void *arg) | MeSmartServo |
flush() (defined in SoftwareSerial) | SoftwareSerial | virtual
getAngleRequest(uint8_t devId) | MeSmartServo |
getCurrentRequest(uint8_t devId) | MeSmartServo |
getPort(void) | MePort |
getSlot(void) | MePort |
getSpeedRequest(uint8_t devId) | MeSmartServo |
getTempRequest(uint8_t devId) | MeSmartServo |
getValue(String key) (defined in MeSerial) | MeSerial |
getVoltageRequest(uint8_t devId) | MeSmartServo |
handle_interrupt() __attribute__((__always_inline__)) (defined in SoftwareSerial) | SoftwareSerial | inline static
handSharke(uint8_t dev_id) | MeSmartServo |
isListening(void) | MeSerial |
lastLine (defined in MeSerial) | MeSerial | protected
letterOf(int i, String s) (defined in MeSerial) | MeSerial |
listen(void) | MeSerial |
MePort(void) | MePort |
MePort(uint8_t port) | MePort |
MePort(uint8_t port, uint8_t slot) | MePort |
MeSerial(void) | MeSerial |
MeSerial(uint8_t port) | MeSerial |
MeSerial(uint8_t receivePin, uint8_t transmitPin, bool inverse_logic=false) | MeSerial |
MeSmartServo() | MeSmartServo |
MeSmartServo(uint8_t port) | MeSmartServo |
move(uint8_t dev_id, long angle_value, float speed, smartServoCb callback=NULL) | MeSmartServo |
moveTo(uint8_t dev_id, long angle_value, float speed, smartServoCb callback=NULL) | MeSmartServo |
operator bool() (defined in SoftwareSerial) | SoftwareSerial | inline
overflow() (defined in SoftwareSerial) | SoftwareSerial | inline
peek() (defined in SoftwareSerial) | SoftwareSerial |
pin(void) | MePort |
pin(uint8_t port, uint8_t slot) | MePort |
pin1(void) | MePort |
pin2(void) | MePort |
poll(void) | MeSerial |
printf(char *fmt,...) | MeSerial |
processSysexMessage(void) | MeSmartServo |
read() | MeSerial | virtual
readByte(uint8_t *argv, int16_t idx) | MeSmartServo |
readDataLine(void) (defined in MeSerial) | MeSerial |
readFloat(uint8_t *argv, int16_t idx) | MeSmartServo |
readLong(uint8_t *argv, int idx) | MeSmartServo |
readShort(uint8_t *argv, int16_t idx, boolean ignore_high) | MeSmartServo |
reset(uint8_t port) | MePort |
reset(uint8_t port, uint8_t slot) | MePort |
s1 | MePort | protected
s2 | MePort | protected
sendByte(uint8_t val) | MeSmartServo |
sendFloat(float val) | MeSmartServo |
sendLong(long val) | MeSmartServo |
sendShort(int16_t val, boolean ignore_high) | MeSmartServo |
sendString(char *str) | MeSerial |
setBreak(uint8_t dev_id, uint8_t breakStatus) | MeSmartServo |
setHardware(bool mode) | MeSerial |
setInitAngle(uint8_t dev_id, uint8_t=0, int16_t=40) | MeSmartServo |
setPwmMove(uint8_t dev_id, int16_t pwm_value) | MeSmartServo |
setRGBLed(uint8_t dev_id, uint8_t r_value, uint8_t g_value, uint8_t b_value) | MeSmartServo |
setZero(uint8_t dev_id) | MeSmartServo |
smartServoCmdResponse(void *arg) | MeSmartServo |
smartServoEventHandle(void) | MeSmartServo |
SoftwareSerial(uint8_t receivePin, uint8_t transmitPin, bool inverse_logic=false) (defined in SoftwareSerial) | SoftwareSerial |
stopListening() (defined in SoftwareSerial) | SoftwareSerial |
stringLength(String s) (defined in MeSerial) | MeSerial |
write(uint8_t byte) | MeSerial | virtual
~SoftwareSerial() (defined in SoftwareSerial) | SoftwareSerial |