\doxysection{src/\+Me\+Pm25\+Sensor.cpp File Reference}
\hypertarget{_me_pm25_sensor_8cpp}{}\label{_me_pm25_sensor_8cpp}\index{src/MePm25Sensor.cpp@{src/MePm25Sensor.cpp}}


Driver for Me PM2.\+5 sensor device.  


{\ttfamily \#include "{}Me\+Pm25\+Sensor.\+h"{}}\newline
{\ttfamily \#include "{}Me\+Serial.\+h"{}}\newline
Include dependency graph for Me\+Pm25\+Sensor.\+cpp\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=350pt]{_me_pm25_sensor_8cpp__incl}
\end{center}
\end{figure}


\doxysubsection{Detailed Description}
Driver for Me PM2.\+5 sensor device. 

\begin{DoxyAuthor}{Author}
Make\+Block 
\end{DoxyAuthor}
\begin{DoxyVersion}{Version}
V1.\+0.\+0 
\end{DoxyVersion}
\begin{DoxyDate}{Date}
2016/12/13 
\end{DoxyDate}
\begin{DoxyParagraph}{Copyright}
This software is Copyright (C), 2012-\/2016, Make\+Block. Use is subject to license ~\newline
conditions. The main licensing options available are GPL V2 or Commercial\+: ~\newline
 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Open Source Licensing GPL V2}
This is the appropriate option if you want to share the source code of your ~\newline
application with everyone you distribute it to, and you also want to give them ~\newline
the right to share who uses it. If you wish to use this software under Open ~\newline
Source Licensing, you must contribute all your source code to the open source ~\newline
community in accordance with the GPL Version 2 when your application is ~\newline
distributed. See \href{http://www.gnu.org/copyleft/gpl.html}{\texttt{ http\+://www.\+gnu.\+org/copyleft/gpl.\+html}}
\end{DoxyParagraph}
\begin{DoxyParagraph}{Description}
This file is a drive for Smart \doxylink{class_servo}{Servo} device, The Smart \doxylink{class_servo}{Servo} inherited the \doxylink{class_me_serial}{Me\+Serial} class from \doxylink{class_software_serial}{Software\+Serial}.
\end{DoxyParagraph}
\begin{DoxyParagraph}{Method List\+:}

\begin{DoxyEnumerate}
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_a3ab7cc63abcb3d89abf615d3c8f68f78}{Me\+Pm25\+Sensor\+::read\+Pm1\+\_\+0\+Concentration(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_ad4f1efe5497f5e2978fc2a3d2fcfcfe8}{Me\+Pm25\+Sensor\+::read\+Pm2\+\_\+5\+Concentration(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_a3835d73853146cbbedb10bf35b24469a}{Me\+Pm25\+Sensor\+::read\+Pm10\+Concentration(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_aef664694c3ca8512d694795dd704e5a3}{Me\+Pm25\+Sensor\+::read0\+\_\+3\+Num\+In100ml(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_aae4537c8e8a21c6304221193b9f35472}{Me\+Pm25\+Sensor\+::read0\+\_\+5\+Num\+In100ml(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_ad07e4c9369d6def86457816936e4ce1e}{Me\+Pm25\+Sensor\+::read1\+\_\+0\+Num\+In100ml(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_a5e6ad588c26febcdf79d53231d492553}{Me\+Pm25\+Sensor\+::read2\+\_\+5\+Num\+In100ml(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_ac780e647570499912c45802baaee8dc2}{Me\+Pm25\+Sensor\+::read5\+\_\+0\+Num\+In100ml(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_a7abb152fbb1530757a3b4e6994b4a578}{Me\+Pm25\+Sensor\+::read10\+Num\+In100ml(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_af061f8c09a9e3bfb4509f7f8cb6b59c6}{Me\+Pm25\+Sensor\+::set\+Ouput\+Compatibility(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_a15457eb6a96687f86ed148e593a94a33}{Me\+Pm25\+Sensor\+::turn\+On\+Fan\+Laser(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_ae2c91a85f42874ba1f9a4b2cc985ad24}{Me\+Pm25\+Sensor\+::turn\+Off\+Fan\+Laser(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_a98a6e7af47ae69ffd23fdae581aef083}{Me\+Pm25\+Sensor\+::\+Output\+Intime\+On(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_a255b47a6afeeac32f7dd9d50a97241e7}{Me\+Pm25\+Sensor\+::\+Output\+Intime\+Off(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_ac126c70ddc9816cac9eedbb9b4387c33}{Me\+Pm25\+Sensor\+::set\+Output\+Intime\+Period(uint16\+\_\+t settime)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_abcec24407e3cbc74c6e47ca2abdd082a}{Me\+Pm25\+Sensor\+::ask\+For\+Data(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_a8c2cb9ec0e5e254eb20639e3167e9d14}{Me\+Pm25\+Sensor\+::core\+Self\+Test(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_a59a38b9cfb0a6145308dfef3a73db42e}{Me\+Pm25\+Sensor\+::set\+Core\+Self\+Test\+Time(uint8\+\_\+t settime)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_aa25fb8cdc6c8ea19f5d8495a3844fb42}{Me\+Pm25\+Sensor\+::set\+Core\+Efficient(uint8\+\_\+t efficent)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_a17bf2e8a068c549f0be44465735899cb}{Me\+Pm25\+Sensor\+::rxloop(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_af756cb35791d5643cebcac6a7ae06514}{Me\+Pm25\+Sensor\+::returnlen(void)};
\item uint16\+\_\+t \doxylink{class_me_pm25_sensor_ae8e7a458edbc826dd1b75f3d135540bf}{Me\+Pm25\+Sensor\+::returnchecksum(void)};
\end{DoxyEnumerate}
\end{DoxyParagraph}
\begin{DoxyParagraph}{History\+:}

\begin{DoxyPre}
`<Author>`         `<Time>`        `<Version>`        `<Descr>`
Zzipeng         2016/12/13     1.0.0            Build the new.
\end{DoxyPre}
 
\end{DoxyParagraph}
