MakeBlock Drive Updated Updated library for MakeBlock Ranger

Loading...
Searching...
No Matches
MeColorSensor Member List

This is the complete list of members for MeColorSensor, including all inherited members.

_port | MePort | protected
_slot | MePort | protected
aRead1(void) | MePort |
aRead2(void) | MePort |
aWrite1(int16_t value) | MePort |
aWrite2(int16_t value) | MePort |
ColorDataRead(void) | MeColorSensor |
ColorDataReadOnebyOne(void) | MeColorSensor |
ColorIdentify(void) | MeColorSensor |
Device_Address (defined in MeColorSensor) | MeColorSensor |
dpRead1(void) | MePort |
dpRead2(void) | MePort |
dRead1(uint8_t mode=INPUT) | MePort |
dRead2(uint8_t mode=INPUT) | MePort |
dWrite1(bool value) | MePort |
dWrite2(bool value) | MePort |
getPort(void) | MePort |
getSlot(void) | MePort |
MAX(uint8_t r, uint8_t g, uint8_t b) | MeColorSensor |
MeColorSensor(void) | MeColorSensor |
MeColorSensor(uint8_t port) | MeColorSensor |
MeColorSensor(uint8_t port, uint8_t address) | MeColorSensor |
MePort(void) | MePort |
MePort(uint8_t port) | MePort |
MePort(uint8_t port, uint8_t slot) | MePort |
MIN(uint8_t r, uint8_t g, uint8_t b) | MeColorSensor |
pin(void) | MePort |
pin(uint8_t port, uint8_t slot) | MePort |
pin1(void) | MePort |
pin2(void) | MePort |
readData(uint8_t start, uint8_t *buffer, uint8_t size) | MeColorSensor |
ReportId(void) | MeColorSensor |
reset(uint8_t port) | MePort |
reset(uint8_t port, uint8_t slot) | MePort |
ReturnBlueData(void) | MeColorSensor |
ReturnColorCode(void) | MeColorSensor |
ReturnColorData(void) | MeColorSensor |
ReturnColorhue(void) | MeColorSensor |
ReturnGrayscale(void) | MeColorSensor |
ReturnGreenData(void) | MeColorSensor |
ReturnRedData(void) | MeColorSensor |
Returnresult(void) | MeColorSensor |
s1 | MePort | protected
s2 | MePort | protected
SensorInit(void) | MeColorSensor |
TurnOffLight(void) | MeColorSensor |
TurnOffmodule(void) | MeColorSensor |
TurnOnLight(void) | MeColorSensor |
TurnOnmodule(void) | MeColorSensor |
writeData(uint8_t start, const uint8_t *pData, uint8_t size) | MeColorSensor |
writeReg(int16_t reg, uint8_t data) | MeColorSensor |