MakeBlock Drive Updated Updated library for MakeBlock Ranger

Loading...
Searching...
No Matches
MeEncoderMotor Member List

This is the complete list of members for MeEncoderMotor, including all inherited members.

_port | MePort | protected
aRead1(void) | MePort |
aRead2(void) | MePort |
aWrite1(int16_t value) | MePort |
aWrite2(int16_t value) | MePort |
begin() | MeEncoderMotor |
dpRead1(void) | MePort |
dpRead2(void) | MePort |
dRead1(uint8_t mode=INPUT) | MePort |
dRead2(uint8_t mode=INPUT) | MePort |
dWrite1(bool value) | MePort |
dWrite2(bool value) | MePort |
getCurrentPosition() | MeEncoderMotor |
getCurrentSpeed() | MeEncoderMotor |
getPort(void) | MePort |
getSlot(void) | MePort |
MeEncoderMotor(uint8_t addr, uint8_t slot) | MeEncoderMotor |
MeEncoderMotor(uint8_t slot) | MeEncoderMotor |
MeEncoderMotor() | MeEncoderMotor |
MePort(void) | MePort |
MePort(uint8_t port) | MePort |
MePort(uint8_t port, uint8_t slot) | MePort |
move(float angle, float speed) | MeEncoderMotor |
moveTo(float angle, float speed) | MeEncoderMotor |
pin(void) | MePort |
pin(uint8_t port, uint8_t slot) | MePort |
pin1(void) | MePort |
pin2(void) | MePort |
reset() | MeEncoderMotor |
MePort::reset(uint8_t port) | MePort |
MePort::reset(uint8_t port, uint8_t slot) | MePort |
runSpeed(float speed) | MeEncoderMotor |
runSpeedAndTime(float speed, float time) | MeEncoderMotor |
runTurns(float turns, float speed) | MeEncoderMotor |
s1 | MePort | protected
s2 | MePort | protected