MakeBlock Drive Updated Updated library for MakeBlock Ranger

Loading...
Searching...
No Matches
MeCompass Member List

This is the complete list of members for MeCompass, including all inherited members.

_port | MePort | protected
_slot | MePort | protected
aRead1(void) | MePort |
aRead2(void) | MePort |
aWrite1(int16_t value) | MePort |
aWrite2(int16_t value) | MePort |
begin(void) | MeCompass |
dpRead1(void) | MePort |
dpRead2(void) | MePort |
dRead1(uint8_t mode=INPUT) | MePort |
dRead2(uint8_t mode=INPUT) | MePort |
dWrite1(bool value) | MePort |
dWrite2(bool value) | MePort |
getAngle(void) | MeCompass |
getHeading(int16_t *x, int16_t *y, int16_t *z) | MeCompass |
getHeadingX(void) | MeCompass |
getHeadingY(void) | MeCompass |
getHeadingZ(void) | MeCompass |
getPort(void) | MePort |
getSlot(void) | MePort |
MeCompass() | MeCompass |
MeCompass(uint8_t port) | MeCompass |
MeCompass(uint8_t port, uint8_t address) | MeCompass |
MePort(void) | MePort |
MePort(uint8_t port) | MePort |
MePort(uint8_t port, uint8_t slot) | MePort |
pin(void) | MePort |
pin(uint8_t port, uint8_t slot) | MePort |
pin1(void) | MePort |
pin2(void) | MePort |
reset(uint8_t port) | MePort |
reset(uint8_t port, uint8_t slot) | MePort |
s1 | MePort | protected
s2 | MePort | protected
setpin(uint8_t keyPin, uint8_t ledPin) | MeCompass |
testConnection(void) | MeCompass |