MakeBlock Drive Updated Updated library for MakeBlock Ranger

Loading...
Searching...
No Matches
MeLEDMatrix Member List

This is the complete list of members for MeLEDMatrix, including all inherited members.

_port | MePort | protected
_slot | MePort | protected
aRead1(void) | MePort |
aRead2(void) | MePort |
aWrite1(int16_t value) | MePort |
aWrite2(int16_t value) | MePort |
clearScreen() | MeLEDMatrix |
dpRead1(void) | MePort |
dpRead2(void) | MePort |
drawBitmap(int8_t x, int8_t y, uint8_t Bitmap_Width, uint8_t *Bitmap) | MeLEDMatrix |
drawStr(int16_t X_position, int8_t Y_position, const char *str) | MeLEDMatrix |
dRead1(uint8_t mode=INPUT) | MePort |
dRead2(uint8_t mode=INPUT) | MePort |
dWrite1(bool value) | MePort |
dWrite2(bool value) | MePort |
getPort(void) | MePort |
getSlot(void) | MePort |
MeLEDMatrix() | MeLEDMatrix |
MeLEDMatrix(uint8_t port) | MeLEDMatrix |
MeLEDMatrix(uint8_t SCK_Pin, uint8_t DIN_Pin) | MeLEDMatrix |
MePort(void) | MePort |
MePort(uint8_t port) | MePort |
MePort(uint8_t port, uint8_t slot) | MePort |
pin(void) | MePort |
pin(uint8_t port, uint8_t slot) | MePort |
pin1(void) | MePort |
pin2(void) | MePort |
reset(uint8_t port) | MeLEDMatrix |
MePort::reset(uint8_t port, uint8_t slot) | MePort |
s1 | MePort | protected
s2 | MePort | protected
setBrightness(uint8_t Bright) | MeLEDMatrix |
setColorIndex(bool Color_Number) | MeLEDMatrix |
showClock(uint8_t hour, uint8_t minute, bool=PointOn) | MeLEDMatrix |
showNum(float value, uint8_t=3) | MeLEDMatrix |