\doxysection{src/\+Me\+Mega\+Pi\+Pro\+ESCMotor.cpp File Reference}
\hypertarget{_me_mega_pi_pro_e_s_c_motor_8cpp}{}\label{_me_mega_pi_pro_e_s_c_motor_8cpp}\index{src/MeMegaPiProESCMotor.cpp@{src/MeMegaPiProESCMotor.cpp}}


Driver for Me Megapipro ESC motor device.  


{\ttfamily \#include "{}Me\+Mega\+Pi\+Pro\+ESCMotor.\+h"{}}\newline
Include dependency graph for Me\+Mega\+Pi\+Pro\+ESCMotor.\+cpp\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=350pt]{_me_mega_pi_pro_e_s_c_motor_8cpp__incl}
\end{center}
\end{figure}


\doxysubsection{Detailed Description}
Driver for Me Megapipro ESC motor device. 

\begin{DoxyAuthor}{Author}
Make\+Block 
\end{DoxyAuthor}
\begin{DoxyVersion}{Version}
V1.\+0.\+2 
\end{DoxyVersion}
\begin{DoxyDate}{Date}
2017/05/22 
\end{DoxyDate}
\begin{DoxyParagraph}{Copyright}
This software is Copyright (C), 2012-\/2017, Make\+Block. Use is subject to license ~\newline
conditions. The main licensing options available are GPL V2 or Commercial\+: ~\newline
 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Open Source Licensing GPL V2}
This is the appropriate option if you want to share the source code of your ~\newline
application with everyone you distribute it to, and you also want to give them ~\newline
the right to share who uses it. If you wish to use this software under Open ~\newline
Source Licensing, you must contribute all your source code to the open source ~\newline
community in accordance with the GPL Version 2 when your application is ~\newline
distributed. See \href{http://www.gnu.org/copyleft/gpl.html}{\texttt{ http\+://www.\+gnu.\+org/copyleft/gpl.\+html}}
\end{DoxyParagraph}
\begin{DoxyParagraph}{Description}
This file is a drive for Me Megapipro ESC mtor device.
\end{DoxyParagraph}
\begin{DoxyParagraph}{Method List\+:}

\end{DoxyParagraph}

\begin{DoxyEnumerate}
\item void \doxylink{class_me_mega_pi_pro_e_s_c_motor_aed9f1a9466a577ec01330e3f1759f3f4}{Me\+Mega\+Pi\+Pro\+ESCMotor\+::setpin(uint8\+\_\+t pwm\+\_\+pin)}
\item void \doxylink{class_me_mega_pi_pro_e_s_c_motor_a7a247a91f39356e7e84200727f13abc1}{Me\+Mega\+Pi\+Pro\+ESCMotor\+::run(int16\+\_\+t speed)}
\item void \doxylink{class_me_mega_pi_pro_e_s_c_motor_ad270cf24ae74e70c946094a0fe86f6ee}{Me\+Mega\+Pi\+Pro\+ESCMotor\+::stop(void)}
\item void \doxylink{class_me_mega_pi_pro_e_s_c_motor_ad9e731bb9c8c3244b11c0d2014e64005}{Me\+Mega\+Pi\+Pro\+ESCMotor\+::reset(uint8\+\_\+t port)}
\end{DoxyEnumerate}

\begin{DoxyParagraph}{History\+:}

\begin{DoxyPre}
`<Author>`         `<Time>`        `<Version>`        `<Descr>`
Lan weiting         2017/05/09       1.0.0            Rebuild the new.
Zzipeng             2017/05/12       1.0.1            add some details.
Zzipeng             2017/05/22       1.0.2            limit bldc speed at 50\% throttle.
\end{DoxyPre}
 
\end{DoxyParagraph}
