MakeBlock Drive Updated Updated library for MakeBlock Ranger

Loading...
Searching...
No Matches
Classes | Macros
MePm25Sensor.h File Reference

Header for for MePm25Sensor.cpp module. More...

`#include <stdint.h>`
`#include <stdbool.h>`
`#include <Arduino.h>`
`#include "MeConfig.h"`
`#include "MeSerial.h"`
`#include "MePort.h"`
Include dependency graph for MePm25Sensor.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Classes
struct | PM25DATASTRUCT
union | PM25DATAUINO
class | MePm25Sensor
| Driver for Me PM2.5 sensor device. More...

## Macros
#define | START_SYSEX1 0x32
#define | START_SYSEX2 0x3d
#define | LENGTH 28

## Detailed Description

Header for for MePm25Sensor.cpp module.

Author
  MakeBlock

Version
  V1.0.0

Date
  2016/12/12

Copyright
  This software is Copyright (C), 2012-2016, MakeBlock. Use is subject to license
  conditions. The main licensing options available are GPL V2 or Commercial:

Open Source Licensing GPL V2
  This is the appropriate option if you want to share the source code of your
  application with everyone you distribute it to, and you also want to give them
  the right to share who uses it. If you wish to use this software under Open
  Source Licensing, you must contribute all your source code to the open source
  community in accordance with the GPL Version 2 when your application is
  distributed. See http://www.gnu.org/copyleft/gpl.html

Description
  This file is a drive for Smart Servo device, The Smart Servo inherited the MeSerial class from SoftwareSerial.

Method List:
  1. uint16_t MePm25Sensor::readPm1_0Concentration(void);
  2. uint16_t MePm25Sensor::readPm2_5Concentration(void);
  3. uint16_t MePm25Sensor::readPm10Concentration(void);
  4. uint16_t MePm25Sensor::read0_3NumIn100ml(void);
  5. uint16_t MePm25Sensor::read0_5NumIn100ml(void);
  6. uint16_t MePm25Sensor::read1_0NumIn100ml(void);
  7. uint16_t MePm25Sensor::read2_5NumIn100ml(void);
  8. uint16_t MePm25Sensor::read5_0NumIn100ml(void);
  9. uint16_t MePm25Sensor::read10NumIn100ml(void);
  10. uint16_t MePm25Sensor::setOuputCompatibility(void);
  11. uint16_t MePm25Sensor::turnOnFanLaser(void);
  12. uint16_t MePm25Sensor::turnOffFanLaser(void);
  13. uint16_t MePm25Sensor::OutputIntimeOn(void);
  14. uint16_t MePm25Sensor::OutputIntimeOff(void);
  15. uint16_t MePm25Sensor::setOutputIntimePeriod(uint16_t settime);
  16. uint16_t MePm25Sensor::askForData(void);
  17. uint16_t MePm25Sensor::coreSelfTest(void);
  18. uint16_t MePm25Sensor::setCoreSelfTestTime(uint8_t settime);
  19. uint16_t MePm25Sensor::setCoreEfficient(uint8_t efficent);
  20. uint16_t MePm25Sensor::rxloop(void);
  21. uint16_t MePm25Sensor::returnlen(void);
  22. uint16_t MePm25Sensor::returnchecksum(void);

History:

      `<Author>`         `<Time>`        `<Version>`        `<Descr>`
      Zzipeng          2016/12/13     1.0.0            Build the new.