\doxysection{src/\+Me\+Infrared\+Receiver.cpp File Reference}
\hypertarget{_me_infrared_receiver_8cpp}{}\label{_me_infrared_receiver_8cpp}\index{src/MeInfraredReceiver.cpp@{src/MeInfraredReceiver.cpp}}


Driver for Me Infrared Receiver device.  


{\ttfamily \#include "{}Me\+Infrared\+Receiver.\+h"{}}\newline
Include dependency graph for Me\+Infrared\+Receiver.\+cpp\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=350pt]{_me_infrared_receiver_8cpp__incl}
\end{center}
\end{figure}


\doxysubsection{Detailed Description}
Driver for Me Infrared Receiver device. 

\begin{DoxyAuthor}{Author}
Make\+Block 
\end{DoxyAuthor}
\begin{DoxyVersion}{Version}
V1.\+0.\+1 
\end{DoxyVersion}
\begin{DoxyDate}{Date}
2017/04/06 
\end{DoxyDate}
\begin{DoxyParagraph}{Copyright}
This software is Copyright (C), 2012-\/2016, Make\+Block. Use is subject to license ~\newline
conditions. The main licensing options available are GPL V2 or Commercial\+: ~\newline
 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Open Source Licensing GPL V2}
This is the appropriate option if you want to share the source code of your ~\newline
application with everyone you distribute it to, and you also want to give them ~\newline
the right to share who uses it. If you wish to use this software under Open ~\newline
Source Licensing, you must contribute all your source code to the open source ~\newline
community in accordance with the GPL Version 2 when your application is ~\newline
distributed. See \href{http://www.gnu.org/copyleft/gpl.html}{\texttt{ http\+://www.\+gnu.\+org/copyleft/gpl.\+html}}
\end{DoxyParagraph}
\begin{DoxyParagraph}{Description}
Description\+: this file is a drive for Me Infrared Receiver, It supports Infrared Receiver V2.\+0 and V3.\+0 device provided by the Make\+Block company.
\end{DoxyParagraph}
\begin{DoxyParagraph}{Method List\+:}

\end{DoxyParagraph}

\begin{DoxyEnumerate}
\item void \doxylink{class_me_infrared_receiver_ac25056e96b50a1bf16c05eedbfeaaf78}{Me\+Infrared\+Receiver\+::begin(void)}
\item int16\+\_\+t \doxylink{class_me_infrared_receiver_aaccf198c3a013b38e783a3e055631110}{Me\+Infrared\+Receiver\+::read(void)}
\item bool \doxylink{class_me_infrared_receiver_a85d4066f35e6838f24e6d3f23a5236a1}{Me\+Infrared\+Receiver\+::button\+State(void)}
\item uint8\+\_\+t \doxylink{class_me_infrared_receiver_a2b4385744d5ff2cd325f15095d257126}{Me\+Infrared\+Receiver\+::get\+Code(void)}
\item void \doxylink{class_me_infrared_receiver_ab178d4d0bb7a3af0aa35a88183c2f928}{Me\+Infrared\+Receiver\+::loop(void)}
\end{DoxyEnumerate}

\begin{DoxyParagraph}{History\+:}

\begin{DoxyPre}
`<Author>`         `<Time>`        `<Version>`        `<Descr>`
Mark Yan         2015/09/09     1.0.0            Rebuild the old lib.
Mark Yan         2017/04/06     1.0.1            Filter out the 0 value of infrared remote.
\end{DoxyPre}
 
\end{DoxyParagraph}
