\doxysection{src/\+Me\+Serial.cpp File Reference}
\hypertarget{_me_serial_8cpp}{}\label{_me_serial_8cpp}\index{src/MeSerial.cpp@{src/MeSerial.cpp}}


this file is a drive for serial  


{\ttfamily \#include "{}Me\+Serial.\+h"{}}\newline
{\ttfamily \#include $<$stdio.\+h$>$}\newline
{\ttfamily \#include $<$stdarg.\+h$>$}\newline
Include dependency graph for Me\+Serial.\+cpp\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=350pt]{_me_serial_8cpp__incl}
\end{center}
\end{figure}


\doxysubsection{Detailed Description}
this file is a drive for serial 

\begin{DoxyAuthor}{Author}
Make\+Block 
\end{DoxyAuthor}
\begin{DoxyVersion}{Version}
V1.\+0.\+3 
\end{DoxyVersion}
\begin{DoxyDate}{Date}
2016/09/20 
\end{DoxyDate}
\begin{DoxyParagraph}{Copyright}
This software is Copyright (C), 2012-\/2016, Make\+Block. Use is subject to license ~\newline
conditions. The main licensing options available are GPL V2 or Commercial\+: ~\newline
 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Open Source Licensing GPL V2}
This is the appropriate option if you want to share the source code of your ~\newline
application with everyone you distribute it to, and you also want to give them ~\newline
the right to share who uses it. If you wish to use this software under Open ~\newline
Source Licensing, you must contribute all your source code to the open source ~\newline
community in accordance with the GPL Version 2 when your application is ~\newline
distributed. See \href{http://www.gnu.org/copyleft/gpl.html}{\texttt{ http\+://www.\+gnu.\+org/copyleft/gpl.\+html}}
\end{DoxyParagraph}
\begin{DoxyParagraph}{Description}
This file is a drive for serial, It support hardware and software serial
\end{DoxyParagraph}
\begin{DoxyParagraph}{Method List\+:}

\end{DoxyParagraph}

\begin{DoxyEnumerate}
\item void \doxylink{class_me_serial_a73dde79161f876956fd6d070f14510d3}{Me\+Serial\+::set\+Hardware(bool mode)}
\item void \doxylink{class_me_serial_a2e491a6206475d8d254a785043e0de22}{Me\+Serial\+::begin(long baudrate)}
\item void \doxylink{class_me_serial_abd68e3efb8adfcc71089dadbd4acd143}{Me\+Serial\+::end(void)}
\item size\+\_\+t \doxylink{class_me_serial_ad28782e0bebe4255a8ba7995957176e6}{Me\+Serial\+::write(uint8\+\_\+t byte)}
\item int16\+\_\+t \doxylink{class_me_serial_a00be49316c437fdb4615c4e40869ff60}{Me\+Serial\+::read(void)}
\item int16\+\_\+t \doxylink{class_me_serial_a4b784a1b24df5e06f208d697e9e1ed3f}{Me\+Serial\+::available(void)}
\item bool \doxylink{class_me_serial_a5dd4784d18202db78fb8333afd97c031}{Me\+Serial\+::listen(void)}
\item bool \doxylink{class_me_serial_a4c4af893caafb362da7906ddabe16327}{Me\+Serial\+::is\+Listening(void)}
\item int16\+\_\+t \doxylink{class_me_serial_a721bd751d68b01eeafd206163eab10a4}{Me\+Serial\+::poll(void)}
\end{DoxyEnumerate}

\begin{DoxyParagraph}{History\+:}

\begin{DoxyPre}
`<Author>`         `<Time>`        `<Version>`        `<Descr>`
Mark Yan         2015/09/08     1.0.0            Rebuild the old lib.
Mark Yan         2016/01/20     1.0.1            support arduino pin-\/setting.
Scott wang       2016/09/18     1.0.2            support the ATmega2560  Serial3 setting.
Scott            2016/09/20     1.0.3            support the Auriga Serial.
\end{DoxyPre}
 
\end{DoxyParagraph}
