MakeBlock Drive Updated Updated library for MakeBlock Ranger

Loading...
Searching...
No Matches
Public Member Functions | List of all members
MePotentiometer Class Reference

Driver for Me potentiometer module. More...

`#include <src/MePotentiometer.h>`

Inheritance diagram for MePotentiometer:
[legend]
Collaboration diagram for MePotentiometer:
[legend]

## Public Member Functions
| MePotentiometer (void)
| MePotentiometer (uint8_t port)
void | setpin (uint8_t potentiometerPin)
uint16_t | read (void)
Public Member Functions inherited from MePort
| MePort (void)
| MePort (uint8_t port)
| MePort (uint8_t port, uint8_t slot)
uint8_t | getPort (void)
uint8_t | getSlot (void)
bool | dRead1 (uint8_t mode=INPUT)
bool | dRead2 (uint8_t mode=INPUT)
bool | dpRead1 (void)
bool | dpRead2 (void)
void | dWrite1 (bool value)
void | dWrite2 (bool value)
int16_t | aRead1 (void)
int16_t | aRead2 (void)
void | aWrite1 (int16_t value)
void | aWrite2 (int16_t value)
void | reset (uint8_t port)
void | reset (uint8_t port, uint8_t slot)
uint8_t | pin1 (void)
uint8_t | pin2 (void)
uint8_t | pin (void)
uint8_t | pin (uint8_t port, uint8_t slot)

## Additional Inherited Members
Protected Attributes inherited from MePort
uint8_t | s1
uint8_t | s2
uint8_t | _port
uint8_t | _slot

## Detailed Description

Driver for Me potentiometer module.

Class: MePotentiometer

Description
  Declaration of Class MePotentiometer.

Copyright (C), 2012-2016, MakeBlock

## Constructor & Destructor Documentation

## ◆ MePotentiometer() [1/2]

MePotentiometer::MePotentiometer | ( | void |  | ) |

Alternate Constructor which can call your own function to map the Me potentiometer device to arduino port, no pins are used or initialized here.

Parameters

  [in] | None |

## ◆ MePotentiometer() [2/2]

MePotentiometer::MePotentiometer | ( | uint8_t | port | ) |

Alternate Constructor which can call your own function to map the Me potentiometer device to arduino port

Parameters

  [in] | port | - RJ25 port from PORT_1 to M2

## Member Function Documentation

## ◆ read()

uint16_t MePotentiometer::read | ( | void |  | ) |

Function
  read()

Description
  Read DAC value of Me potentiometer module.

Parameters

  [in] | None |

Output
  None

Return
  The value of potentiometer device(0-1024)

Others
  None

## ◆ setpin()

void MePotentiometer::setpin | ( | uint8_t | potentiometerPin | ) |

Function
  setpin

Description
  Reset the potentiometer device available PIN by its arduino port.

Parameters

  [in] | potentiometerPin | - arduino port for potentiometer output port

Output
  None

Return
  None

Others
  None

The documentation for this class was generated from the following files:

- src/MePotentiometer.h
- src/MePotentiometer.cpp