\doxysection{Me\+Light\+Sensor Class Reference}
\hypertarget{class_me_light_sensor}{}\label{class_me_light_sensor}\index{MeLightSensor@{MeLightSensor}}


Driver for Me-\/\+Light Sensor module.  




{\ttfamily \#include $<$src/\+Me\+Light\+Sensor.\+h$>$}



Inheritance diagram for Me\+Light\+Sensor\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=161pt]{class_me_light_sensor__inherit__graph}
\end{center}
\end{figure}


Collaboration diagram for Me\+Light\+Sensor\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=161pt]{class_me_light_sensor__coll__graph}
\end{center}
\end{figure}
\doxysubsubsection*{Public Member Functions}
\begin{DoxyCompactItemize}
\item 
\mbox{\hyperlink{class_me_light_sensor_a369148767eeac2ad59e724554621298d}{Me\+Light\+Sensor}} (void)
\item 
\mbox{\hyperlink{class_me_light_sensor_af7e3e21af2ea0190d65655750bf49665}{Me\+Light\+Sensor}} (uint8\+\_\+t port)
\item 
void \mbox{\hyperlink{class_me_light_sensor_a9b4ca3d8caf6c4dcc2de651dddb37ce6}{setpin}} (uint8\+\_\+t led\+Pin, uint8\+\_\+t sensor\+Pin)
\item 
int16\+\_\+t \mbox{\hyperlink{class_me_light_sensor_aaae9be2df39ab2c86c4b27c618e3fb48}{read}} (void)
\item 
void \mbox{\hyperlink{class_me_light_sensor_aab0e6ecb7bb432e9e131811fabac77c3}{light\+On}} (void)
\item 
void \mbox{\hyperlink{class_me_light_sensor_a0b787d14763d3c34e353ff6f6ef9b3f8}{light\+Off}} (void)
\end{DoxyCompactItemize}
\doxysubsection*{Public Member Functions inherited from \mbox{\hyperlink{class_me_port}{Me\+Port}}}
\begin{DoxyCompactItemize}
\item 
\mbox{\hyperlink{class_me_port_ae4b9e8e718b626d0ce4017a430878210}{Me\+Port}} (void)
\item 
\mbox{\hyperlink{class_me_port_a7a1d7cdf061740148cd893ba481420a3}{Me\+Port}} (uint8\+\_\+t port)
\item 
\mbox{\hyperlink{class_me_port_a1458b606f98da409d7ab4fa7d09c6816}{Me\+Port}} (uint8\+\_\+t port, uint8\+\_\+t slot)
\item 
uint8\+\_\+t \mbox{\hyperlink{class_me_port_a8d9ca22e35477573b27c4165ac61def0}{get\+Port}} (void)
\item 
uint8\+\_\+t \mbox{\hyperlink{class_me_port_a4c73dec349340e958b9567b06fa6f27c}{get\+Slot}} (void)
\item 
bool \mbox{\hyperlink{class_me_port_a8b7b990f5fa85dfc28f7f3d0d7ba46b9}{d\+Read1}} (uint8\+\_\+t mode=INPUT)
\item 
bool \mbox{\hyperlink{class_me_port_ab4fd13565335bd781da8f44bae803031}{d\+Read2}} (uint8\+\_\+t mode=INPUT)
\item 
bool \mbox{\hyperlink{class_me_port_aabcb0e1dc89942cf302b8cbac2cbd0a5}{dp\+Read1}} (void)
\item 
bool \mbox{\hyperlink{class_me_port_a2e4b6faf3e9494e819ccee47dfb8010e}{dp\+Read2}} (void)
\item 
void \mbox{\hyperlink{class_me_port_a9d5f60427202c26bc8da4b1e6a66c5c2}{d\+Write1}} (bool value)
\item 
void \mbox{\hyperlink{class_me_port_a0d9ee041f8361f45bcc83bed9577415f}{d\+Write2}} (bool value)
\item 
int16\+\_\+t \mbox{\hyperlink{class_me_port_acfd28b1ab8cc6af5bf8223446022525c}{a\+Read1}} (void)
\item 
int16\+\_\+t \mbox{\hyperlink{class_me_port_a63709dcbe9850c0d3baec1fed72809bf}{a\+Read2}} (void)
\item 
void \mbox{\hyperlink{class_me_port_adb4d7959f2059bf9986a8e5a631988ae}{a\+Write1}} (int16\+\_\+t value)
\item 
void \mbox{\hyperlink{class_me_port_a3834f0f30618ec31789d524dd367e44f}{a\+Write2}} (int16\+\_\+t value)
\item 
void \mbox{\hyperlink{class_me_port_a7b82ce913d98ecff906569d795073892}{reset}} (uint8\+\_\+t port)
\item 
void \mbox{\hyperlink{class_me_port_a91e3cca62e5f8fffead56f8104488d4d}{reset}} (uint8\+\_\+t port, uint8\+\_\+t slot)
\item 
uint8\+\_\+t \mbox{\hyperlink{class_me_port_a1ed16a0f863a618cc9f32b27015107e7}{pin1}} (void)
\item 
uint8\+\_\+t \mbox{\hyperlink{class_me_port_a8a1b3cd06dffbb48d40c3adf25011803}{pin2}} (void)
\item 
uint8\+\_\+t \mbox{\hyperlink{class_me_port_aea7dad0142d940c0395b1782fe5adeae}{pin}} (void)
\item 
uint8\+\_\+t \mbox{\hyperlink{class_me_port_a637d42b5a62d655b8517bc8a363206f3}{pin}} (uint8\+\_\+t port, uint8\+\_\+t slot)
\end{DoxyCompactItemize}
\doxysubsubsection*{Additional Inherited Members}
\doxysubsection*{Protected Attributes inherited from \mbox{\hyperlink{class_me_port}{Me\+Port}}}
\begin{DoxyCompactItemize}
\item 
uint8\+\_\+t \mbox{\hyperlink{class_me_port_ab5295b9e84ecedf3f93ab47cf8f10284}{s1}}
\item 
uint8\+\_\+t \mbox{\hyperlink{class_me_port_a6c09cece23372a6ab340512a0db3e37d}{s2}}
\item 
uint8\+\_\+t \mbox{\hyperlink{class_me_port_adc9cdd4e574061d41244fc662974544f}{\+\_\+port}}
\item 
uint8\+\_\+t \mbox{\hyperlink{class_me_port_a4159543b593b047cd82fedab30b178b7}{\+\_\+slot}}
\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
Driver for Me-\/\+Light Sensor module. 

Class\+: \doxylink{class_me_light_sensor}{Me\+Light\+Sensor} \begin{DoxyParagraph}{Description}
Declaration of Class \doxylink{class_me_light_sensor}{Me\+Light\+Sensor}.
\end{DoxyParagraph}
\begin{DoxyParagraph}{Copyright (C), 2012-\/2016, Make\+Block}

\end{DoxyParagraph}


\doxysubsection{Constructor \& Destructor Documentation}
\Hypertarget{class_me_light_sensor_a369148767eeac2ad59e724554621298d}\label{class_me_light_sensor_a369148767eeac2ad59e724554621298d} 
\index{MeLightSensor@{MeLightSensor}!MeLightSensor@{MeLightSensor}}
\index{MeLightSensor@{MeLightSensor}!MeLightSensor@{MeLightSensor}}
\doxysubsubsection{\texorpdfstring{MeLightSensor()}{MeLightSensor()}\hspace{0.1cm}{\footnotesize\ttfamily [1/2]}}
{\footnotesize\ttfamily Me\+Light\+Sensor\+::\+Me\+Light\+Sensor (\begin{DoxyParamCaption}\item[{void}]{ }\end{DoxyParamCaption})}

Alternate Constructor which can call your own function to map the light sensor to arduino port, no pins are used or initialized here. 
\begin{DoxyParams}[1]{Parameters}
\mbox{\texttt{ in}}  & {\em None} & \\
\hline
\end{DoxyParams}
\Hypertarget{class_me_light_sensor_af7e3e21af2ea0190d65655750bf49665}\label{class_me_light_sensor_af7e3e21af2ea0190d65655750bf49665} 
\index{MeLightSensor@{MeLightSensor}!MeLightSensor@{MeLightSensor}}
\index{MeLightSensor@{MeLightSensor}!MeLightSensor@{MeLightSensor}}
\doxysubsubsection{\texorpdfstring{MeLightSensor()}{MeLightSensor()}\hspace{0.1cm}{\footnotesize\ttfamily [2/2]}}
{\footnotesize\ttfamily Me\+Light\+Sensor\+::\+Me\+Light\+Sensor (\begin{DoxyParamCaption}\item[{uint8\+\_\+t}]{port }\end{DoxyParamCaption})}

Alternate Constructor which can call your own function to map the light sensor to arduino port 
\begin{DoxyParams}[1]{Parameters}
\mbox{\texttt{ in}}  & {\em port} & -\/ RJ25 port from PORT\+\_\+1 to M2 \\
\hline
\end{DoxyParams}


\doxysubsection{Member Function Documentation}
\Hypertarget{class_me_light_sensor_a0b787d14763d3c34e353ff6f6ef9b3f8}\label{class_me_light_sensor_a0b787d14763d3c34e353ff6f6ef9b3f8} 
\index{MeLightSensor@{MeLightSensor}!lightOff@{lightOff}}
\index{lightOff@{lightOff}!MeLightSensor@{MeLightSensor}}
\doxysubsubsection{\texorpdfstring{lightOff()}{lightOff()}}
{\footnotesize\ttfamily void Me\+Light\+Sensor\+::light\+Off (\begin{DoxyParamCaption}\item[{void}]{ }\end{DoxyParamCaption})}

\begin{DoxyParagraph}{Function}
light\+Off 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Description}
Turn off the LED on the light sensor. 
\end{DoxyParagraph}

\begin{DoxyParams}[1]{Parameters}
\mbox{\texttt{ in}}  & {\em None} & \\
\hline
\end{DoxyParams}
\begin{DoxyParagraph}{Output}
None 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Return}
None 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Others}

\end{DoxyParagraph}
\Hypertarget{class_me_light_sensor_aab0e6ecb7bb432e9e131811fabac77c3}\label{class_me_light_sensor_aab0e6ecb7bb432e9e131811fabac77c3} 
\index{MeLightSensor@{MeLightSensor}!lightOn@{lightOn}}
\index{lightOn@{lightOn}!MeLightSensor@{MeLightSensor}}
\doxysubsubsection{\texorpdfstring{lightOn()}{lightOn()}}
{\footnotesize\ttfamily void Me\+Light\+Sensor\+::light\+On (\begin{DoxyParamCaption}\item[{void}]{ }\end{DoxyParamCaption})}

\begin{DoxyParagraph}{Function}
light\+On 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Description}
Turn on the LED on the light sensor. 
\end{DoxyParagraph}

\begin{DoxyParams}[1]{Parameters}
\mbox{\texttt{ in}}  & {\em None} & \\
\hline
\end{DoxyParams}
\begin{DoxyParagraph}{Output}
None 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Return}
None 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Others}

\end{DoxyParagraph}
\Hypertarget{class_me_light_sensor_aaae9be2df39ab2c86c4b27c618e3fb48}\label{class_me_light_sensor_aaae9be2df39ab2c86c4b27c618e3fb48} 
\index{MeLightSensor@{MeLightSensor}!read@{read}}
\index{read@{read}!MeLightSensor@{MeLightSensor}}
\doxysubsubsection{\texorpdfstring{read()}{read()}}
{\footnotesize\ttfamily int16\+\_\+t Me\+Light\+Sensor\+::read (\begin{DoxyParamCaption}\item[{void}]{ }\end{DoxyParamCaption})}

\begin{DoxyParagraph}{Function}
read 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Description}
Read analog value of light sensor. 
\end{DoxyParagraph}

\begin{DoxyParams}[1]{Parameters}
\mbox{\texttt{ in}}  & {\em None} & \\
\hline
\end{DoxyParams}
\begin{DoxyParagraph}{Output}
None 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Return}
\doxylink{class_me_port_a63709dcbe9850c0d3baec1fed72809bf}{Me\+Port\+::a\+Read2()} -\/ DAC value of current light sensor\textquotesingle{}s output. 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Others}

\end{DoxyParagraph}
\Hypertarget{class_me_light_sensor_a9b4ca3d8caf6c4dcc2de651dddb37ce6}\label{class_me_light_sensor_a9b4ca3d8caf6c4dcc2de651dddb37ce6} 
\index{MeLightSensor@{MeLightSensor}!setpin@{setpin}}
\index{setpin@{setpin}!MeLightSensor@{MeLightSensor}}
\doxysubsubsection{\texorpdfstring{setpin()}{setpin()}}
{\footnotesize\ttfamily void Me\+Light\+Sensor\+::setpin (\begin{DoxyParamCaption}\item[{uint8\+\_\+t}]{led\+Pin,  }\item[{uint8\+\_\+t}]{sensor\+Pin }\end{DoxyParamCaption})}

\begin{DoxyParagraph}{Function}
setpin 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Description}
Set I2C data pin, clock pin and clear display. ~\newline
 data\+Pin -\/ the DATA pin for Seven-\/\+Segment LED module. ~\newline
 clk\+Pin -\/ the CLK pin for Seven-\/\+Segment LED module. 
\end{DoxyParagraph}

\begin{DoxyParams}[1]{Parameters}
\mbox{\texttt{ in}}  & {\em led\+Pin} & -\/ Which pin on board that LEDpin is connecting to. \\
\hline
\mbox{\texttt{ in}}  & {\em sensor\+Pin} & -\/ Which pin on board that sensor\+Pin is connecting to. \\
\hline
\end{DoxyParams}
\begin{DoxyParagraph}{Output}
None 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Return}
None 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Others}
Set global variable \+\_\+\+Key\+Pin and s2 
\end{DoxyParagraph}


The documentation for this class was generated from the following files\+:\begin{DoxyCompactItemize}
\item 
src/\mbox{\hyperlink{_me_light_sensor_8h}{Me\+Light\+Sensor.\+h}}\item 
src/\mbox{\hyperlink{_me_light_sensor_8cpp}{Me\+Light\+Sensor.\+cpp}}\end{DoxyCompactItemize}
