# Esp32_8ServoUnitWifiGC

The sketch uses:
- M5Stack 8ServoUnit to drive servos, see:https://shop.m5stack.com/products/8-channel-servo-driver-unit-stm32f030
- ServoEasing library
- WifiGC to allow connecting to an OpenLCB hub, such as available in JMRI.

It also demonstrates:
- Multiple easing function, selectable in the CDI
- A user definited easing function
- Servo endpoint adjustment in the CDI

<img src="https://github.com/user-attachments/assets/a1c13062-c06e-4efd-82f5-0814fe9367bc" alt="M5Stack 8Servo Unit" width="300">

