
OLED
http://code.google.com/p/u8glib/

Install instructions for the Arduino environment.

  1. Start Arduino IDE
  2. In the Arduino IDE, import the library from the "Add Library" Menu.

Alternative install instructions for the Arduino environment.

  1. Unzip u8glib_arduino_vX.XX.zip into the "libraries" folder of the
      Arduino install directory
  2. Start Arduino IDE

Install instructions for the Chipkit (Arduino) environment.

  1. cd <mpide-... path>/libraries
  2. unzip u8glib_arduino_vX.XX.zip
  3. cd <mpide-... path>///hardware/pic32/libraries
  4. again: u8glib_arduino_vX.XX.zip
  5. Open hardware/pic32/cores/pic32/Print.h
	  Remove line
	    #define BYTE 0
	  from the file, use PRINT_BYTE instead of BYTE. 
	