#######################################
# Syntax Coloring Map
#######################################
# https://arduino.github.io/arduino-cli/0.21/library-specification/#keywordstxt-format
# KEYWORD1 Classes, datatypes, and C++ keywords
# KEYWORD2 Methods and functions
# KEYWORD3 setup and loop functions, as well as the Serial keywords
# LITERAL1 Constants
# LITERAL2 Built-in variables (unused by default)


################################################
# Classes, datatypes (KEYWORD1)
################################################
UFC23									KEYWORD1
ufc23									KEYWORD1

################################################
# Methods and Functions (KEYWORD2)
################################################
begin									KEYWORD2
isConnected								KEYWORD2

init									KEYWORD2
update									KEYWORD2
reset									KEYWORD2
stopMeasurement							KEYWORD2
updateConfiguration						KEYWORD2
readConfig								KEYWORD2
writeConfig								KEYWORD2
setConfigurationRegisters				KEYWORD2
startMeasurement						KEYWORD2
hasError								KEYWORD2
getErrors								KEYWORD2
isMeasuring								KEYWORD2
errorToStrings							KEYWORD2
partIdToString							KEYWORD2
readCommunicationFlags					KEYWORD2
readInterruptFlags						KEYWORD2
readFrontendErrorFlags					KEYWORD2
readFrontendStatusFlags					KEYWORD2
readSystemStatusFlags					KEYWORD2
clearFlags								KEYWORD2
triggerSingleMeasurement				KEYWORD2
sendRemoteCommand						KEYWORD2
readRamAddress							KEYWORD2
writeRamAddress							KEYWORD2
getAmplitudeMeasurementResultsRaw		KEYWORD2
getAmplitudeMeasurementResultsV			KEYWORD2
getPulseWidthMeasurementResultsRaw		KEYWORD2
getPulseWidthMeasurementResultsRatio	KEYWORD2
getMultiHitSumNs						KEYWORD2
getMultiHitCount						KEYWORD2
getVddVcc								KEYWORD2
getHighSpeedOscillatorFrequencyMhz		KEYWORD2
getZeroCrossLevelV						KEYWORD2
getTemperaturesSeq1DegC					KEYWORD2
getTemperaturesSeq2DegC					KEYWORD2
getIndividualTofHitsNs					KEYWORD2
getAverageHitNs							KEYWORD2
getSupplyVoltageV						KEYWORD2
getHighSpeedClockFrequencyHz			KEYWORD2
triggerSpoolPortOpenCheck				KEYWORD2
isSpoolWorkingWell						KEYWORD2

################################################
# Constants (LITERAL1)
################################################
CONSTANT								LITERAL1

