semilimes mcu sdk 1.1.3 semilimes Software Development Kit for microcontrollers

Loading...
Searching...
No Matches
Public Member Functions | Public Attributes | List of all members
FcQrScanner Class Reference

## Public Member Functions
| ~FcQrScanner ()
void | set (const char *refname, const char *title, bool reqSel, const char *value, const char *actBtnTitle, const char *mode)
char * | get ()

## Public Attributes
char | mode [3][8] = {"auto","qrcode","barcode"}

## Constructor & Destructor Documentation

## ◆ ~FcQrScanner()

FcQrScanner::~FcQrScanner | ( |  | ) |
| inline

Returns
  void

## Member Function Documentation

## ◆ get()

char * FcQrScanner::get | ( |  | ) |

Returns
  char*

## ◆ set()

void FcQrScanner::set | ( | const char * | refname,
|  | const char * | title,
|  | bool | reqSel,
|  | const char * | value,
|  | const char * | actBtnTitle,
|  | const char * | mode )

Parameters

  refname | - it is the reference name of the object
  title | - is the text displayed next to the scanner
  reqSel | - indicates if the selection is required to submit the form
  value | - is the decoded value of the NFC scan upon form submission
  actBtnTitle | - is the label of the scan button
  mode | - selects the type of code to support. Allowed values: auto, qrcode, barcode. char mode[3][8] = {"auto","qrcode","barcode"};

Returns
  void

## Member Data Documentation

## ◆ mode

char FcQrScanner::mode[3][8] = {"auto","qrcode","barcode"}

Parameters

  char | mode[3][8] = {"auto","qrcode","barcode"};

The documentation for this class was generated from the following files:

- C:/Users/flavio_unige/Desktop/semilimes/sdk/semilimes MCU SDK/github/semilimes_mcu_sdk/src/components/fc_qr_scanner.h
- C:/Users/flavio_unige/Desktop/semilimes/sdk/semilimes MCU SDK/github/semilimes_mcu_sdk/src/components/fc_qr_scanner.cpp