Macros | Functions
example_service_sensor_disable.c File Reference
`#include <stdbool.h>`
`#include <stdint.h>`
`#include <stdio.h>`
`#include <stdlib.h>`
`#include "acc_config.h"`
`#include "acc_definitions_a121.h"`
`#include "acc_definitions_common.h"`
`#include "acc_hal_definitions_a121.h"`
`#include "acc_hal_integration_a121.h"`
`#include "acc_integration.h"`
`#include "acc_processing.h"`
`#include "acc_rss_a121.h"`
`#include "acc_sensor.h"`
`#include "acc_version.h"`

Go to the source code of this file.

## Macros
#define | SENSOR_ID (1U)
#define | SENSOR_TIMEOUT_MS (1000U)
#define | MAX_DATA_ENTRY_LEN 15

## Functions
static void | set_config (acc_config_t *config)
static void | print_data (acc_int16_complex_t *data, uint16_t data_length)
static void | cleanup (acc_config_t *config, acc_processing_t *processing, acc_sensor_t *sensor, void *buffer)
int | acconeer_main (int argc, char *argv[])
| Assembly test example. More...

## Macro Definition Documentation

## ◆ MAX_DATA_ENTRY_LEN

#define MAX_DATA_ENTRY_LEN 15

Examples
  example_service_sensor_disable.c.

Definition at line 45 of file example_service_sensor_disable.c.

## ◆ SENSOR_ID

#define SENSOR_ID (1U)

Examples
  example_service_sensor_disable.c.

Definition at line 43 of file example_service_sensor_disable.c.

## ◆ SENSOR_TIMEOUT_MS

#define SENSOR_TIMEOUT_MS (1000U)

Examples
  example_service_sensor_disable.c.

Definition at line 44 of file example_service_sensor_disable.c.

## Function Documentation

## ◆ acconeer_main()

int acconeer_main | ( | int | argc,
|  | char * | argv[]
| ) |  |

Assembly test example.

Surface velocity example application.

Tank level reference application.

Smart presence reference application.

Breathing example application.

Service subsweeps example.

Service multple configurations example.

Low power service example.

Service example.

Processing subtract adaptive background example.

Processing static presence example.

Processing peak interpolation example.

Processing noncoherent mean example.

Processing coherent mean example.

Processing amplitude example.

Detector presence example with multiple configurations.

Low power detector presence example.

Detector presence example.

Distance detector low power example.

Detector distance example.

Control helper example.

Returns
  Returns EXIT_SUCCESS if successful, otherwise EXIT_FAILURE

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Examples
  example_service_sensor_disable.c.

Definition at line 61 of file example_service_sensor_disable.c.

## ◆ cleanup()

static void cleanup | ( | acc_config_t * | config,
|  | acc_processing_t * | processing,
|  | acc_sensor_t * | sensor,
|  | void * | buffer
| ) |  |
| static

Examples
  example_service_sensor_disable.c.

Definition at line 206 of file example_service_sensor_disable.c.

## ◆ print_data()

static void print_data | ( | acc_int16_complex_t * | data,
|  | uint16_t | data_length
| ) |  |
| static

Examples
  example_service_sensor_disable.c.

Definition at line 234 of file example_service_sensor_disable.c.

## ◆ set_config()

static void set_config | ( | acc_config_t * | config | ) |
| static

Examples
  example_service_sensor_disable.c.

Definition at line 255 of file example_service_sensor_disable.c.