Functions
example_service.h File Reference

Go to the source code of this file.

## Functions
int | acconeer_main (int argc, char *argv[])
| Service example. More...

## Function Documentation

## ◆ acconeer_main()

int acconeer_main | ( | int | argc,
|  | char * | argv[]
| ) |  |

Service example.

Returns
  Returns EXIT_SUCCESS if successful, otherwise EXIT_FAILURE

Service example.

Processing subtract adaptive background example.

Processing static presence example.

Processing peak interpolation example.

Processing noncoherent mean example.

Processing coherent mean example.

Processing amplitude example.

Detector presence example with multiple configurations.

Low power detector presence example.

Detector presence example.

Distance detector low power example.

Detector distance example.

Control helper example.

Returns
  Returns EXIT_SUCCESS if successful, otherwise EXIT_FAILURE

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Definition at line 245 of file acc_exploration_server_stm32.c.