Macros | Functions
example_service.c File Reference
`#include <stdbool.h>`
`#include <stdint.h>`
`#include <stdio.h>`
`#include <stdlib.h>`
`#include "acc_config.h"`
`#include "acc_definitions_a121.h"`
`#include "acc_definitions_common.h"`
`#include "acc_hal_definitions_a121.h"`
`#include "acc_hal_integration_a121.h"`
`#include "acc_integration.h"`
`#include "acc_processing.h"`
`#include "acc_rss_a121.h"`
`#include "acc_sensor.h"`
`#include "acc_version.h"`

Go to the source code of this file.

## Macros
#define | SENSOR_ID (1U)
#define | SENSOR_TIMEOUT_MS (1000U)
#define | MAX_DATA_ENTRY_LEN (15U)

## Functions
static void | set_config (acc_config_t *config)
static bool | do_sensor_calibration_and_prepare (acc_sensor_t *sensor, acc_config_t *config, void *buffer, uint32_t buffer_size)
static void | print_data (acc_int16_complex_t *data, uint16_t data_length)
static void | cleanup (acc_config_t *config, acc_processing_t *processing, acc_sensor_t *sensor, void *buffer)
int | acconeer_main (int argc, char *argv[])
| Assembly test example. More...

## Macro Definition Documentation

## ◆ MAX_DATA_ENTRY_LEN

#define MAX_DATA_ENTRY_LEN (15U)

Examples
  example_service.c.

Definition at line 43 of file example_service.c.

## ◆ SENSOR_ID

#define SENSOR_ID (1U)

Examples
  example_service.c.

Definition at line 41 of file example_service.c.

## ◆ SENSOR_TIMEOUT_MS

#define SENSOR_TIMEOUT_MS (1000U)

Examples
  example_service.c.

Definition at line 42 of file example_service.c.

## Function Documentation

## ◆ acconeer_main()

int acconeer_main | ( | int | argc,
|  | char * | argv[]
| ) |  |

Assembly test example.

Surface velocity example application.

Tank level reference application.

Smart presence reference application.

Breathing example application.

Service subsweeps example.

Service multple configurations example.

Low power service example.

Service example.

Processing subtract adaptive background example.

Processing static presence example.

Processing peak interpolation example.

Processing noncoherent mean example.

Processing coherent mean example.

Processing amplitude example.

Detector presence example with multiple configurations.

Low power detector presence example.

Detector presence example.

Distance detector low power example.

Detector distance example.

Control helper example.

Returns
  Returns EXIT_SUCCESS if successful, otherwise EXIT_FAILURE

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Examples
  example_service.c.

Definition at line 61 of file example_service.c.

## ◆ cleanup()

static void cleanup | ( | acc_config_t * | config,
|  | acc_processing_t * | processing,
|  | acc_sensor_t * | sensor,
|  | void * | buffer
| ) |  |
| static

Examples
  example_service.c.

Definition at line 264 of file example_service.c.

## ◆ do_sensor_calibration_and_prepare()

static bool do_sensor_calibration_and_prepare | ( | acc_sensor_t * | sensor,
|  | acc_config_t * | config,
|  | void * | buffer,
|  | uint32_t | buffer_size
| ) |  |
| static

Examples
  example_service.c.

Definition at line 205 of file example_service.c.

## ◆ print_data()

static void print_data | ( | acc_int16_complex_t * | data,
|  | uint16_t | data_length
| ) |  |
| static

Examples
  example_service.c.

Definition at line 243 of file example_service.c.

## ◆ set_config()

static void set_config | ( | acc_config_t * | config | ) |
| static

Examples
  example_service.c.

Definition at line 196 of file example_service.c.