### - m -

- M_PI : acc_alg_basic_utils.h
- MAIN_UART_HANDLE : main.h
- MAX_DATA_ENTRY_LEN : example_service_low_power_sensor_hibernate.c , example_service_sensor_off.c , example_service_subsweeps.c , example_service_multiple_configurations.c , example_control_helper.c , example_service.c , example_service_low_power_sensor_disable.c , example_service_sensor_disable.c , example_service_sensor_hibernate.c
- MAX_DATA_ENTRY_LEN_FLOAT : acc_processing_helpers.c
- MAX_DATA_ENTRY_LEN_IQ : acc_processing_helpers.c
- MCU_INT_GPIO_Port : main.h
- MCU_INT_Pin : main.h
- MEDIUM_TANK_CLOSE_RANGE_LEAKAGE_CANCELLATION : ref_app_tank_level.c
- MEDIUM_TANK_MAX_PROFILE : ref_app_tank_level.c
- MEDIUM_TANK_MAX_STEP_LENGTH : ref_app_tank_level.c
- MEDIUM_TANK_MEDIAN_FILTER_LENGTH : ref_app_tank_level.c
- MEDIUM_TANK_NUM_FRAMES_REC : ref_app_tank_level.c
- MEDIUM_TANK_NUM_MEDIANS_TO_AVERAGE : ref_app_tank_level.c
- MEDIUM_TANK_PEAK_SORTING : ref_app_tank_level.c
- MEDIUM_TANK_RANGE_END_M : ref_app_tank_level.c
- MEDIUM_TANK_RANGE_START_M : ref_app_tank_level.c
- MEDIUM_TANK_REFLECTOR_SHAPE : ref_app_tank_level.c
- MEDIUM_TANK_SIGNAL_QUALITY : ref_app_tank_level.c
- MEDIUM_TANK_THRESHOLD_SENSITIVITY : ref_app_tank_level.c
- MIN_PEAK_VS : example_surface_velocity.c
- MISC_GPIO0_GPIO_Port : main.h
- MISC_GPIO0_Pin : main.h
- MISC_GPIO1_GPIO_Port : main.h
- MISC_GPIO1_Pin : main.h
- MISC_GPIO2_GPIO_Port : main.h
- MISC_GPIO2_Pin : main.h
- MODULE : acc_exploration_server_stm32.c
- MODULE_I2C_HANDLE : main.h
- MODULE_RTC_HANDLE : main.h
- MODULE_UART1_HANDLE : main.h
- MODULE_UART2_HANDLE : main.h
- MSI_VALUE : stm32l4xx_hal_conf.h