Macros | Enumerations | Functions
example_detector_presence_low_power_off.c File Reference
`#include <stdbool.h>`
`#include <stdint.h>`
`#include <stdio.h>`
`#include <stdlib.h>`
`#include "acc_definitions_a121.h"`
`#include "acc_definitions_common.h"`
`#include "acc_detector_presence.h"`
`#include "acc_hal_definitions_a121.h"`
`#include "acc_hal_integration_a121.h"`
`#include "acc_integration.h"`
`#include "acc_rss_a121.h"`
`#include "acc_sensor.h"`
`#include "acc_version.h"`

Go to the source code of this file.

## Macros
#define | SENSOR_ID (1U)
#define | SENSOR_TIMEOUT_MS (1000U)
#define | DEFAULT_PRESET_CONFIG PRESENCE_PRESET_CONFIG_MEDIUM_RANGE

## Enumerations
enum | presence_preset_config_t { PRESENCE_PRESET_CONFIG_NONE = 0, PRESENCE_PRESET_CONFIG_SHORT_RANGE, PRESENCE_PRESET_CONFIG_MEDIUM_RANGE, PRESENCE_PRESET_CONFIG_LONG_RANGE, PRESENCE_PRESET_CONFIG_LOW_POWER_WAKEUP, PRESENCE_PRESET_CONFIG_NONE = 0, PRESENCE_PRESET_CONFIG_SHORT_RANGE, PRESENCE_PRESET_CONFIG_MEDIUM_RANGE, PRESENCE_PRESET_CONFIG_LONG_RANGE, PRESENCE_PRESET_CONFIG_LOW_POWER_WAKEUP, PRESENCE_PRESET_CONFIG_NONE = 0, PRESENCE_PRESET_CONFIG_SHORT_RANGE, PRESENCE_PRESET_CONFIG_MEDIUM_RANGE, PRESENCE_PRESET_CONFIG_LONG_RANGE }

## Functions
static void | print_result (acc_detector_presence_result_t result)
static void | cleanup (acc_detector_presence_handle_t *presence_handle, acc_detector_presence_config_t *presence_config, acc_sensor_t *sensor, void *buffer)
static void | set_config (acc_detector_presence_config_t *presence_config, presence_preset_config_t preset)
int | acconeer_main (int argc, char *argv[])
| Assembly test example. More...

## Macro Definition Documentation

## ◆ DEFAULT_PRESET_CONFIG

#define DEFAULT_PRESET_CONFIG PRESENCE_PRESET_CONFIG_MEDIUM_RANGE

Examples
  example_detector_presence_low_power_off.c.

Definition at line 61 of file example_detector_presence_low_power_off.c.

## ◆ SENSOR_ID

#define SENSOR_ID (1U)

Examples
  example_detector_presence_low_power_off.c.

Definition at line 58 of file example_detector_presence_low_power_off.c.

## ◆ SENSOR_TIMEOUT_MS

#define SENSOR_TIMEOUT_MS (1000U)

Examples
  example_detector_presence_low_power_off.c.

Definition at line 59 of file example_detector_presence_low_power_off.c.

## Enumeration Type Documentation

## ◆ presence_preset_config_t

enum presence_preset_config_t

Enumerator
PRESENCE_PRESET_CONFIG_NONE |
PRESENCE_PRESET_CONFIG_SHORT_RANGE |
PRESENCE_PRESET_CONFIG_MEDIUM_RANGE |
PRESENCE_PRESET_CONFIG_LONG_RANGE |
PRESENCE_PRESET_CONFIG_LOW_POWER_WAKEUP |
PRESENCE_PRESET_CONFIG_NONE |
PRESENCE_PRESET_CONFIG_SHORT_RANGE |
PRESENCE_PRESET_CONFIG_MEDIUM_RANGE |
PRESENCE_PRESET_CONFIG_LONG_RANGE |
PRESENCE_PRESET_CONFIG_LOW_POWER_WAKEUP |
PRESENCE_PRESET_CONFIG_NONE |
PRESENCE_PRESET_CONFIG_SHORT_RANGE |
PRESENCE_PRESET_CONFIG_MEDIUM_RANGE |
PRESENCE_PRESET_CONFIG_LONG_RANGE |

Examples
  example_detector_presence_low_power_off.c.

Definition at line 48 of file example_detector_presence_low_power_off.c.

## Function Documentation

## ◆ acconeer_main()

int acconeer_main | ( | int | argc,
|  | char * | argv[]
| ) |  |

Assembly test example.

Surface velocity example application.

Tank level reference application.

Smart presence reference application.

Breathing example application.

Service subsweeps example.

Service multple configurations example.

Low power service example.

Service example.

Processing subtract adaptive background example.

Processing static presence example.

Processing peak interpolation example.

Processing noncoherent mean example.

Processing coherent mean example.

Processing amplitude example.

Detector presence example with multiple configurations.

Low power detector presence example.

Detector presence example.

Distance detector low power example.

Detector distance example.

Control helper example.

Returns
  Returns EXIT_SUCCESS if successful, otherwise EXIT_FAILURE

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Examples
  example_detector_presence_low_power_off.c.

Definition at line 79 of file example_detector_presence_low_power_off.c.

## ◆ cleanup()

static void cleanup | ( | acc_detector_presence_handle_t * | presence_handle,
|  | acc_detector_presence_config_t * | presence_config,
|  | acc_sensor_t * | sensor,
|  | void * | buffer
| ) |  |
| static

Examples
  example_detector_presence_low_power_off.c.

Definition at line 226 of file example_detector_presence_low_power_off.c.

## ◆ print_result()

static void print_result | ( | acc_detector_presence_result_t | result | ) |
| static

Examples
  example_detector_presence_low_power_off.c.

Definition at line 372 of file example_detector_presence_low_power_off.c.

## ◆ set_config()

static void set_config | ( | acc_detector_presence_config_t * | presence_config,
|  | presence_preset_config_t | preset
| ) |  |
| static

Examples
  example_detector_presence_low_power_off.c.

Definition at line 256 of file example_detector_presence_low_power_off.c.