acc_hal_integration_a121.h
Go to the documentation of this file.
1 // Copyright (c) Acconeer AB, 2021-2022
2 // All rights reserved
3
4 #ifndef ACC_HAL_INTEGRATION_A121_H_
5 #define ACC_HAL_INTEGRATION_A121_H_
6
7 #include <stdbool.h>
8 #include <stdint.h>
9
10 #include "acc_definitions_common.h"
11 #include "acc_hal_definitions_a121.h"
12
13
14 /**
15 * @brief Get hal implementation reference
16 */
17 const acc_hal_a121_t *acc_hal_rss_integration_get_implementation(void);
18
19
20 /**
21 * @brief Power on sensor supply
22 *
23 * @param[in] sensor_id The id of the sensor to power on
24 */
25 void acc_hal_integration_sensor_supply_on(acc_sensor_id_t sensor_id);
26
27
28 /**
29 * @brief Power off sensor supply
30 *
31 * @param[in] sensor_id The id of the sensor to power off
32 */
33 void acc_hal_integration_sensor_supply_off(acc_sensor_id_t sensor_id);
34
35
36 /**
37 * @brief Enable sensor
38 *
39 * Any pending sensor interrupts should be cleared before returning from function.
40 * The sensor supply needs to be enabled by invoking @ref acc_hal_integration_sensor_supply_on
41 * before calling this function.
42 *
43 * @param[in] sensor_id The id of the sensor to enable
44 */
45 void acc_hal_integration_sensor_enable(acc_sensor_id_t sensor_id);
46
47
48 /**
49 * @brief Disable sensor
50 *
51 * @param[in] sensor_id The id of the sensor to disable
52 */
53 void acc_hal_integration_sensor_disable(acc_sensor_id_t sensor_id);
54
55
56 /**
57 * @brief Wait for a sensor interrupt
58 *
59 * @param[in] sensor_id The sensor to wait for the interrupt on
60 * @param[in] timeout_ms The maximum time to wait in milliseconds
61 * @return True if an interrupt has occurred within timeout, false if timeout occurred
62 */
63 bool acc_hal_integration_wait_for_sensor_interrupt(acc_sensor_id_t sensor_id, uint32_t timeout_ms);
64
65
66 /**
67 * @brief Get the max number of sensors the integration supports
68 *
69 * @return The max sensor count
70 */
71 uint16_t acc_hal_integration_sensor_count(void);
72
73
74 #endif
acc_hal_integration_sensor_supply_off
void acc_hal_integration_sensor_supply_off(acc_sensor_id_t sensor_id)
Power off sensor supply.
Definition: acc_hal_integration_stm32cube_xm.c:113
acc_hal_integration_sensor_supply_on
void acc_hal_integration_sensor_supply_on(acc_sensor_id_t sensor_id)
Power on sensor supply.
Definition: acc_hal_integration_stm32cube_xm.c:107
acc_hal_rss_integration_get_implementation
const acc_hal_a121_t * acc_hal_rss_integration_get_implementation(void)
Get hal implementation reference.
Definition: acc_hal_integration_stm32cube_xm.c:166
acc_hal_a121_t
Definition: acc_hal_definitions_a121.h:82
acc_hal_integration_wait_for_sensor_interrupt
bool acc_hal_integration_wait_for_sensor_interrupt(acc_sensor_id_t sensor_id, uint32_t timeout_ms)
Wait for a sensor interrupt.
Definition: acc_hal_integration_stm32cube_xm.c:142
acc_hal_integration_sensor_enable
void acc_hal_integration_sensor_enable(acc_sensor_id_t sensor_id)
Enable sensor.
Definition: acc_hal_integration_stm32cube_xm.c:119
acc_hal_definitions_a121.h
acc_hal_integration_sensor_disable
void acc_hal_integration_sensor_disable(acc_sensor_id_t sensor_id)
Disable sensor.
Definition: acc_hal_integration_stm32cube_xm.c:130
acc_sensor_id_t
uint32_t acc_sensor_id_t
Type representing a sensor ID.
Definition: acc_definitions_common.h:14
acc_hal_integration_sensor_count
uint16_t acc_hal_integration_sensor_count(void)
Get the max number of sensors the integration supports.
Definition: acc_hal_integration_stm32cube_xm.c:185
acc_definitions_common.h