AFE_NXP_Arduino 1.0.3 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Here is a list of all class members with links to the classes they belong to:

### - a -

- AFE_base() : AFE_base
- afe_ptr : LogicalChannel_Base

### - b -

- begin() : AFE_base
- bit_count() : AFE_base
- bit_op() : NAFE13388_Base
- blink_leds() : NAFE13388_Base, NAFE13388_UIM
- boot() : AFE_base, NAFE13388_Base
- burst() : SPI_for_AFE

### - c -

- cal_index : NAFE13388_Base::_ref_points
- calc_delay() : NAFE13388_Base
- CalibrationError : NAFE13388_Base
- callback_fp_t : AFE_base
- cbf_DRDY : AFE_base
- ch_delay : AFE_base
- ch_number : LogicalChannel_Base
- ch_setting_t : NAFE13388_Base
- channel_info_update() : NAFE13388_Base
- close_logical_channel() : AFE_base, NAFE13388_Base
- CMD_ABORT : NAFE13388_Base
- CMD_BURST_DATA : NAFE13388_Base
- CMD_CALC_CRC_COEF : NAFE13388_Base
- CMD_CALC_CRC_CONFG : NAFE13388_Base
- CMD_CALC_CRC_FAC : NAFE13388_Base
- CMD_CH0 : NAFE13388_Base
- CMD_CH1 : NAFE13388_Base
- CMD_CH10 : NAFE13388_Base
- CMD_CH11 : NAFE13388_Base
- CMD_CH12 : NAFE13388_Base
- CMD_CH13 : NAFE13388_Base
- CMD_CH14 : NAFE13388_Base
- CMD_CH15 : NAFE13388_Base
- CMD_CH2 : NAFE13388_Base
- CMD_CH3 : NAFE13388_Base
- CMD_CH4 : NAFE13388_Base
- CMD_CH5 : NAFE13388_Base
- CMD_CH6 : NAFE13388_Base
- CMD_CH7 : NAFE13388_Base
- CMD_CH8 : NAFE13388_Base
- CMD_CH9 : NAFE13388_Base
- CMD_CLEAR_ALARM : NAFE13388_Base
- CMD_CLEAR_DATA : NAFE13388_Base
- CMD_CLEAR_REG : NAFE13388_Base
- CMD_END : NAFE13388_Base
- CMD_MC : NAFE13388_Base
- CMD_MM : NAFE13388_Base
- CMD_MS : NAFE13388_Base
- CMD_RELOAD : NAFE13388_Base
- CMD_RESET : NAFE13388_Base
- CMD_SC : NAFE13388_Base
- CMD_SS : NAFE13388_Base
- coeff_index : NAFE13388_Base::_ref_points
- coeff_mV() : AFE_base
- coeff_uV : AFE_base
- Command : NAFE13388_Base
- command() : NAFE13388_Base
- command_length : SPI_for_AFE
- configure() : NAFE13388_Base::LogicalChannel

### - d -

- data : NAFE13388_Base::_reference_point
- default_drdy_cb() : AFE_base
- delay_accuracy : AFE_base
- dev_add : AFE_base
- disable() : LogicalChannel_Base
- DRDY_by_sequencer_done() : AFE_base, NAFE13388_Base
- DRDY_cb() : AFE_base
- drdy_count : AFE_base
- drdy_delay() : AFE_base
- drdy_flag : AFE_base

### - e -

- enable() : LogicalChannel_Base
- enable_logical_channel() : AFE_base, NAFE13388_Base
- enabled_channels : AFE_base
- enabled_logical_channels() : AFE_base

### - g -

- G_PGA_x16_0 : NAFE13388_Base
- G_PGA_x_0_2 : NAFE13388_Base
- G_PGA_x_0_4 : NAFE13388_Base
- G_PGA_x_0_8 : NAFE13388_Base
- G_PGA_x_1_0 : NAFE13388_Base
- G_PGA_x_2_0 : NAFE13388_Base
- G_PGA_x_4_0 : NAFE13388_Base
- G_PGA_x_8_0 : NAFE13388_Base
- gain_offset_coeff() : NAFE13388_Base
- GainError : NAFE13388_Base
- GainPGA : NAFE13388_Base
- get_data16() : SPI_for_AFE
- get_data24() : SPI_for_AFE
- GPIO0_GPIO1 : AFE_base

### - h -

- high : NAFE13388_Base::_ref_points
- highspeed_variant : AFE_base
- HV_MUX : AFE_base

### - i -

- init() : AFE_base
- instance : AFE_base

### - l -

- logical_channel : NAFE13388_Base
- LogicalChannel() : NAFE13388_Base::LogicalChannel
- LogicalChannel_Base() : LogicalChannel_Base
- low : NAFE13388_Base::_ref_points
- LV_mux_sel : AFE_base

### - m -

- microvolt_t : AFE_base
- mux_setting : AFE_base

### - n -

- NAFE13388() : NAFE13388
- NAFE13388_Base() : NAFE13388_Base
- NAFE13388_UIM() : NAFE13388_UIM
- NoError : NAFE13388_Base

### - o -

- OffsetError : NAFE13388_Base
- open_logical_channel() : AFE_base, NAFE13388_Base
- operator AFE_base::microvolt_t() : LogicalChannel_Base
- operator AFE_base::raw_t() : LogicalChannel_Base
- operator*() : LogicalChannel_Base
- operator+() : LogicalChannel_Base
- operator-() : LogicalChannel_Base
- operator/() : LogicalChannel_Base

### - p -

- part_number() : NAFE13388_Base
- pga_gain : NAFE13388_Base
- pin_DRDY : AFE_base
- pin_DRDY_input : AFE_base
- pin_nINT : AFE_base
- pin_nRESET : AFE_base
- pin_SYN : AFE_base

### - r -

- raw2mv() : AFE_base
- raw2uv() : AFE_base
- raw2v() : AFE_base
- raw_t : AFE_base
- read() : AFE_base, LogicalChannel_Base, NAFE13388_Base
- read_r16() : SPI_for_AFE
- read_r24() : SPI_for_AFE
- REF2_REF2 : AFE_base
- REF2_VHSS : AFE_base
- ref_points : NAFE13388_Base
- REFCOARSE_REF2 : AFE_base
- reference_point : NAFE13388_Base
- reg() : NAFE13388_Base
- Register16 : NAFE13388_Base
- Register24 : NAFE13388_Base
- reset() : AFE_base, NAFE13388_Base
- revision_number() : NAFE13388_Base

### - s -

- self_calibrate() : NAFE13388_Base
- sequence_order : AFE_base
- serial_number() : NAFE13388_Base
- set_DRDY_callback() : AFE_base
- start() : AFE_base, NAFE13388_Base
- start_and_read() : AFE_base
- start_continuous_conversion() : AFE_base, NAFE13388_Base
- static_default_drdy_cb() : AFE_base

### - t -

- TBD : NAFE13388_Base
- temperature() : NAFE13388_Base
- timeout_limit : AFE_base
- total_delay : AFE_base
- txrx() : SPI_for_AFE

### - u -

- use_DRDY_trigger() : AFE_base

### - v -

- VADD_REF2 : AFE_base
- VHDD_REF2 : AFE_base
- voltage : NAFE13388_Base::_reference_point

### - w -

- wait_conversion_complete() : AFE_base
- write_r16() : SPI_for_AFE
- write_r24() : SPI_for_AFE

### - ~ -

- ~AFE_base() : AFE_base
- ~LogicalChannel() : NAFE13388_Base::LogicalChannel
- ~LogicalChannel_Base() : LogicalChannel_Base
- ~NAFE13388() : NAFE13388
- ~NAFE13388_Base() : NAFE13388_Base
- ~NAFE13388_UIM() : NAFE13388_UIM