AFE_NXP_Arduino 1.0.3 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Here is a list of all variables with links to the classes they belong to:

- afe_ptr : LogicalChannel_Base
- cal_index : NAFE13388_Base::_ref_points
- cbf_DRDY : AFE_base
- ch_delay : AFE_base
- ch_number : LogicalChannel_Base
- coeff_index : NAFE13388_Base::_ref_points
- coeff_uV : AFE_base
- command_length : SPI_for_AFE
- data : NAFE13388_Base::_reference_point
- delay_accuracy : AFE_base
- dev_add : AFE_base
- drdy_count : AFE_base
- drdy_flag : AFE_base
- enabled_channels : AFE_base
- high : NAFE13388_Base::_ref_points
- highspeed_variant : AFE_base
- instance : AFE_base
- logical_channel : NAFE13388_Base
- low : NAFE13388_Base::_ref_points
- mux_setting : AFE_base
- pga_gain : NAFE13388_Base
- pin_DRDY : AFE_base
- pin_DRDY_input : AFE_base
- pin_nINT : AFE_base
- pin_nRESET : AFE_base
- pin_SYN : AFE_base
- sequence_order : AFE_base
- timeout_limit : AFE_base
- total_delay : AFE_base
- voltage : NAFE13388_Base::_reference_point