AFE_NXP_Arduino 1.0.3 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
LogicalChannel_Base Member List

This is the complete list of members for LogicalChannel_Base, including all inherited members.

afe_ptr | LogicalChannel_Base |
ch_number | LogicalChannel_Base |
disable(void) | LogicalChannel_Base |
enable(void) | LogicalChannel_Base |
LogicalChannel_Base() | LogicalChannel_Base | inline
operator AFE_base::microvolt_t(void) | LogicalChannel_Base |
operator AFE_base::raw_t(void) | LogicalChannel_Base |
operator*(T v) | LogicalChannel_Base | inline
operator*(T v, LogicalChannel_Base lc) | LogicalChannel_Base | friend
operator+(T v) | LogicalChannel_Base | inline
operator+(T v, LogicalChannel_Base lc) | LogicalChannel_Base | friend
operator-(T v) | LogicalChannel_Base | inline
operator-(T v, LogicalChannel_Base lc) | LogicalChannel_Base | friend
operator/(T v) | LogicalChannel_Base | inline
operator/(T v, LogicalChannel_Base lc) | LogicalChannel_Base | friend
read(void) | LogicalChannel_Base |
read(void) | LogicalChannel_Base |
read(void) | LogicalChannel_Base |
~LogicalChannel_Base() | LogicalChannel_Base | inlinevirtual