AFE_NXP_Arduino 1.0.3 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Here is a list of all enum values with links to the classes they belong to:

### - c -

- CMD_ABORT : NAFE13388_Base
- CMD_BURST_DATA : NAFE13388_Base
- CMD_CALC_CRC_COEF : NAFE13388_Base
- CMD_CALC_CRC_CONFG : NAFE13388_Base
- CMD_CALC_CRC_FAC : NAFE13388_Base
- CMD_CH0 : NAFE13388_Base
- CMD_CH1 : NAFE13388_Base
- CMD_CH10 : NAFE13388_Base
- CMD_CH11 : NAFE13388_Base
- CMD_CH12 : NAFE13388_Base
- CMD_CH13 : NAFE13388_Base
- CMD_CH14 : NAFE13388_Base
- CMD_CH15 : NAFE13388_Base
- CMD_CH2 : NAFE13388_Base
- CMD_CH3 : NAFE13388_Base
- CMD_CH4 : NAFE13388_Base
- CMD_CH5 : NAFE13388_Base
- CMD_CH6 : NAFE13388_Base
- CMD_CH7 : NAFE13388_Base
- CMD_CH8 : NAFE13388_Base
- CMD_CH9 : NAFE13388_Base
- CMD_CLEAR_ALARM : NAFE13388_Base
- CMD_CLEAR_DATA : NAFE13388_Base
- CMD_CLEAR_REG : NAFE13388_Base
- CMD_END : NAFE13388_Base
- CMD_MC : NAFE13388_Base
- CMD_MM : NAFE13388_Base
- CMD_MS : NAFE13388_Base
- CMD_RELOAD : NAFE13388_Base
- CMD_RESET : NAFE13388_Base
- CMD_SC : NAFE13388_Base
- CMD_SS : NAFE13388_Base

### - g -

- G_PGA_x16_0 : NAFE13388_Base
- G_PGA_x_0_2 : NAFE13388_Base
- G_PGA_x_0_4 : NAFE13388_Base
- G_PGA_x_0_8 : NAFE13388_Base
- G_PGA_x_1_0 : NAFE13388_Base
- G_PGA_x_2_0 : NAFE13388_Base
- G_PGA_x_4_0 : NAFE13388_Base
- G_PGA_x_8_0 : NAFE13388_Base
- GainError : NAFE13388_Base
- GPIO0_GPIO1 : AFE_base

### - h -

- HV_MUX : AFE_base

### - n -

- NoError : NAFE13388_Base

### - o -

- OffsetError : NAFE13388_Base

### - r -

- REF2_REF2 : AFE_base
- REF2_VHSS : AFE_base
- REFCOARSE_REF2 : AFE_base

### - t -

- TBD : NAFE13388_Base

### - v -

- VADD_REF2 : AFE_base
- VHDD_REF2 : AFE_base