AFE_NXP_Arduino 2.0.0 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Here is a list of all class members with links to the classes they belong to:

### - o -

- OffsetError : NAFE13388_Base
- on_board_shunt_resister : NAFE33352_Base
- open_dac_output() : NAFE33352_Base
- open_logical_channel() : AFE_base, NAFE13388_Base, NAFE33352_Base
- operator AFE_base::raw_t() : LogicalChannel_Base
- operator AFE_base::volt_t() : LogicalChannel_Base
- operator*() : LogicalChannel_Base
- operator+() : LogicalChannel_Base
- operator-() : LogicalChannel_Base
- operator/() : LogicalChannel_Base
- operator=() : NAFE33352_Base::DAC
- output() : NAFE33352_Base::DAC
- output_mode : NAFE33352_Base::DAC