AFE_NXP_Arduino 2.0.0 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Classes | Public Types | Public Member Functions | Public Attributes | Static Public Attributes | Private Member Functions | List of all members
NAFE33352_Base Class Reference

`#include <NAFE33352.h>`

Inheritance diagram for NAFE33352_Base:

## Classes
class | LogicalChannel
class | DAC

## Public Types
enum | IN_SEL : uint8_t { VCM_VCM = 0 , AIP_AIN , AIP_VSNS , GPIO0_GPIO1 , AIP , AIN , ISNS , VSNS , TIA , GPIO0_VCM , VCM_GPIO1 , REF_BYP__VCM , VCM__REF_BYP , BG , VADD , LDO , VHDD , VHSS , DAC_REF }
enum | GainPGA : uint8_t { G_PGA_x_1_0 , G_PGA_x16_0 }
enum class | Register16 : uint16_t { CRC_CONF_REGS = 0x20 , CRC_COEF_REGS = 0x21 , CRC_TRIM_REGS = 0x22 , CRC_TRIM_REF = 0x3F , GPI_DATA = 0x23 , GPO_ENABLE = 0x24 , GPIO_FUNCTION = 0x25 , GPI_ENABLE = 0x26 , GPI_EDGE_POS = 0x27 , GPI_EDGE_NEG = 0x28 , GPO_DATA = 0x29 , SYS_CONFIG = 0x2A , SYS_STATUS = 0x2B , CK_SRC_SEL_CONFIG = 0x30 , GLOBAL_ALARM_ENABLE = 0x2C , GLOBAL_ALARM_INT = 0x2D , DIE_TEMP = 0x2E , TEMP_THRS = 0x2F , PN2 = 0x40 , PN1 = 0x41 , PN0_REV = 0x42 , AI_CONFIG0 = 0x1000 | 0x20 , AI_CONFIG1 = 0x1000 | 0x21 , AI_CONFIG2 = 0x1000 | 0x22 , AI_MULTI_CH_EN = 0x1000 | 0x23 , AI_SYSCFG = 0x1000 | 0x24 , AI_STATUS = 0x1000 | 0x25 , AI_STATUS_OVR = 0x1000 | 0x26 , AI_STATUS_UDR = 0x1000 | 0x27 , AIO_CONFIG = 0x1C00 | 0x20 , AO_CAL_COEF = 0x1C00 | 0x21 , AIO_PROT_CFG = 0x1C00 | 0x22 , AO_SLR_CTRL = 0x1C00 | 0x23 , AWG_PER = 0x1C00 | 0x24 , AO_SYSCFG = 0x1C00 | 0x25 , AIO_STATUS = 0x1C00 | 0x26 }
enum class | Register24 : uint16_t { GAIN_COEF0 = 0x50 , GAIN_COEF1 , GAIN_COEF2 , GAIN_COEF3 , GAIN_COEF4 , GAIN_COEF5 , GAIN_COEF6 , GAIN_COEF7 , OFFSET_COEF0 = 0x58 , OFFSET_COEF1 , OFFSET_COEF2 , OFFSET_COEF3 , OFFSET_COEF4 , OFFSET_COEF5 , OFFSET_COEF6 , OFFSET_COEF7 , EXTRA_CAL_COEF0 = 0x60 , EXTRA_CAL_COEF1 , EXTRA_CAL_COEF2 , EXTRA_CAL_COEF3 , EXTRA_CAL_COEF4 , EXTRA_CAL_COEF5 , EXTRA_CAL_COEF6 , EXTRA_CAL_COEF7 , SERIAL1 = 0x43 , SERIAL0 , AI_DATA0 = 0x1000 | 0x30 , AI_DATA1 , AI_DATA2 , AI_DATA3 , AI_DATA4 , AI_DATA5 , AI_DATA6 , AI_DATA7 , AI_CH_OVR_THR_0 = 0x1000 | 0x38 , AI_CH_OVR_THR_1 , AI_CH_OVR_THR_2 , AI_CH_OVR_THR_3 , AI_CH_OVR_THR_4 , AI_CH_OVR_THR_5 , AI_CH_OVR_THR_6 , AI_CH_OVR_THR_7 , AI_CH_UDR_THR_0 = 0x1000 | 0x40 , AI_CH_UDR_THR_1 , AI_CH_UDR_THR_2 , AI_CH_UDR_THR_3 , AI_CH_UDR_THR_4 , AI_CH_UDR_THR_5 , AI_CH_UDR_THR_6 , AI_CH_UDR_THR_7 , AO_DATA = 0x1C00 | 0x28 , AO_OC_POS_LIMIT , AO_OC_NEG_LIMIT , AWG_AMP_MAX , AWG_AMP_MIN }
enum | Command : uint16_t { CMD_CLEAR_ALARM = 0x12 , CMD_RESET = 0x14 , CMD_CLEAR_REG = 0x15 , CMD_RELOAD = 0x16 , CMD_CALC_CRC_CONFIG = 0x2006 , CMD_CALC_CRC_COEF = 0x2007 , CMD_CALC_CRC_FAC = 0x2008 , CMD_CH0 = 0x1000 , CMD_CH1 = 0x1001 , CMD_CH2 = 0x1002 , CMD_CH3 = 0x1003 , CMD_CH4 = 0x1004 , CMD_CH5 = 0x1005 , CMD_CH6 = 0x1006 , CMD_CH7 = 0x1007 , CMD_ADC_ABORT = 0x1010 , CMD_END = 0x1012 , CMD_CLEAR_DATA = 0x1013 , CMD_SS = 0x3000 , CMD_SC = 0x3001 , CMD_MM = 0x3002 , CMD_MC = 0x3003 , CMD_MS = 0x3004 , CMD_BURST_DATA = 0x3005 , CMD_WGEN_STOP = 0x1C00 , CMD_WGEN_START = 0x1C01 , CMD_CLEAR_DAC0 = 0x1C02 , CMD_AO_ABORT = 0x1C03 , CMD_AO_ABORT_HIZ = 0x1C04 , CMD_CISW_ABORT = 0x1C05 , CMD_CISW_ABORT_HIZ = 0x1C06 }
using | ch_setting_t = uint16_t[ 4 ]
Public Types inherited from AFE_base
enum | LV_mux_sel : uint8_t { REF2_REF2 = 0 , GPIO0_GPIO1 , REFCOARSE_REF2 , VADD_REF2 , VHDD_REF2 , REF2_VHSS , HV_MUX }
using | raw_t = int32_t
using | volt_t = double
typedef void(* | callback_fp_t) (void)

## Public Member Functions
| NAFE33352_Base (bool spi_addr, bool highspeed_variant, int nINT, int DRDY, int SYN, int nRESET, int DRDY_input, int SYNCDAC)
virtual | ~NAFE33352_Base ()
virtual void | boot (void)
virtual void | reset (bool hardware_reset=false)
virtual void | open_logical_channel (int ch, uint16_t cc0, uint16_t cc1, uint16_t cc2, uint16_t dummy)
virtual void | open_logical_channel (int ch, const uint16_t(&cc)[4])
void | open_dac_output (const uint16_t(&cc)[6])
virtual void | close_logical_channel (int ch)
virtual void | close_logical_channel (void)
void | enable_logical_channel (int ch)
virtual void | start (int ch)
virtual void | start (void)
virtual void | start_continuous_conversion ()
virtual void | DRDY_by_sequencer_done (bool flag=true)
virtual raw_t | read (int ch)
virtual void | read (raw_t *data)
virtual void | read (volt_t *data)
double | raw2v (int ch, raw_t value)
virtual void | dac_out (double vi, double full_scale, uint8_t bit_length)
int32_t | dac_code (double a, double full_scale, uint8_t bit_length)
virtual void | command (uint16_t com)
virtual void | reg (Register16 r, uint16_t value)
virtual void | reg (Register24 r, uint32_t value)
virtual uint16_t | reg (Register16 r)
virtual uint32_t | reg (Register24 r)
template<typename T>
uint32_t | bit_op (T rg, uint32_t mask, uint32_t value)
uint64_t | part_number (void)
uint8_t | revision_number (void)
uint64_t | serial_number (void)
float | temperature (void)
Public Member Functions inherited from AFE_base
| AFE_base (bool spi_addr, bool highspeed_variant, int nINT, int DRDY, int SYN, int nRESET, int DRDY_input, int SYNCDAC)
virtual | ~AFE_base ()
virtual void | begin (void)
virtual void | set_DRDY_callback (callback_fp_t fnc)
virtual raw_t | start_and_read (int ch)
template<typename T>
void | start_and_read (T data)
double | raw2uv (int ch, raw_t value)
double | raw2mv (int ch, raw_t value)
double | drdy_delay (int ch)
double | drdy_delay (void)
int | enabled_logical_channels (void)
void | use_DRDY_trigger (bool use=true)
Public Member Functions inherited from SPI_for_AFE
void | txrx (uint8_t *data, int size)
void | write_r16 (uint16_t reg)
void | write_r16 (uint16_t reg, uint16_t val)
uint16_t | read_r16 (uint16_t reg)
void | write_r24 (uint16_t reg, uint32_t val)
int32_t | read_r24 (uint16_t reg)
void | burst (uint32_t *data, int length, int width=3)

## Public Attributes
LogicalChannel | logical_channel [16]
DAC | dac

## Static Public Attributes
static constexpr double | on_board_shunt_resister = 50.00
static constexpr double | pga_gain [] = { 1.00, 16.00 }
Static Public Attributes inherited from AFE_base
static AFE_base * | instance = nullptr

## Private Member Functions
double | calc_delay (int ch)
void | channel_info_update (uint16_t value)

## Additional Inherited Members
Protected Member Functions inherited from AFE_base
int | bit_count (uint32_t value)
void | default_drdy_cb ()
virtual void | init (void)
int | wait_conversion_complete (double delay=-1.0)
Static Protected Member Functions inherited from AFE_base
static void | static_default_drdy_cb ()
static void | DRDY_cb ()
Protected Attributes inherited from AFE_base
bool | dev_add
bool | highspeed_variant
int | pin_nINT
int | pin_DRDY
int | pin_SYN
int | pin_nRESET
int | pin_DRDY_input
int | pin_SYNCDAC
int | enabled_channels
uint8_t | sequence_order [16]
double | coeff_V [16]
int | mux_setting [16]
double | ch_delay [16]
double | total_delay
uint32_t | drdy_count
volatile bool | drdy_flag
Static Protected Attributes inherited from AFE_base
static double | delay_accuracy = 1.2
static constexpr uint32_t | timeout_limit = 10000000
static callback_fp_t | cbf_DRDY = nullptr

## Detailed Description

NXP Analog Front End class library for MCX

Author
  Tedd OKANO

Copyright: 2026 Tedd OKANO Released under the MIT license

Definition at line 16 of file NAFE33352.h.

## Member Typedef Documentation

## ◆ ch_setting_t

using NAFE33352_Base::ch_setting_t = uint16_t[ 4 ]

Definition at line 19 of file NAFE33352.h.

## Member Enumeration Documentation

## ◆ Command

enum NAFE33352_Base::Command : uint16_t

Enumerator
CMD_CLEAR_ALARM |
CMD_RESET |
CMD_CLEAR_REG |
CMD_RELOAD |
CMD_CALC_CRC_CONFIG |
CMD_CALC_CRC_COEF |
CMD_CALC_CRC_FAC |
CMD_CH0 |
CMD_CH1 |
CMD_CH2 |
CMD_CH3 |
CMD_CH4 |
CMD_CH5 |
CMD_CH6 |
CMD_CH7 |
CMD_ADC_ABORT |
CMD_END |
CMD_CLEAR_DATA |
CMD_SS |
CMD_SC |
CMD_MM |
CMD_MC |
CMD_MS |
CMD_BURST_DATA |
CMD_WGEN_STOP |
CMD_WGEN_START |
CMD_CLEAR_DAC0 |
CMD_AO_ABORT |
CMD_AO_ABORT_HIZ |
CMD_CISW_ABORT |
CMD_CISW_ABORT_HIZ |

Definition at line 355 of file NAFE33352.h.

## ◆ GainPGA

enum NAFE33352_Base::GainPGA : uint8_t

Enumerator
G_PGA_x_1_0 |
G_PGA_x16_0 |

Definition at line 249 of file NAFE33352.h.

## ◆ IN_SEL

enum NAFE33352_Base::IN_SEL : uint8_t

Enumerator
VCM_VCM |
AIP_AIN |
AIP_VSNS |
GPIO0_GPIO1 |
AIP |
AIN |
ISNS |
VSNS |
TIA |
GPIO0_VCM |
VCM_GPIO1 |
REF_BYP__VCM |
VCM__REF_BYP |
BG |
VADD |
LDO |
VHDD |
VHSS |
DAC_REF |

Definition at line 227 of file NAFE33352.h.

## ◆ Register16

enum class NAFE33352_Base::Register16 : uint16_t
| strong

Enumerator
CRC_CONF_REGS |
CRC_COEF_REGS |
CRC_TRIM_REGS |
CRC_TRIM_REF |
GPI_DATA |
GPO_ENABLE |
GPIO_FUNCTION |
GPI_ENABLE |
GPI_EDGE_POS |
GPI_EDGE_NEG |
GPO_DATA |
SYS_CONFIG |
SYS_STATUS |
CK_SRC_SEL_CONFIG |
GLOBAL_ALARM_ENABLE |
GLOBAL_ALARM_INT |
DIE_TEMP |
TEMP_THRS |
PN2 |
PN1 |
PN0_REV |
AI_CONFIG0 |
AI_CONFIG1 |
AI_CONFIG2 |
AI_MULTI_CH_EN |
AI_SYSCFG |
AI_STATUS |
AI_STATUS_OVR |
AI_STATUS_UDR |
AIO_CONFIG |
AO_CAL_COEF |
AIO_PROT_CFG |
AO_SLR_CTRL |
AWG_PER |
AO_SYSCFG |
AIO_STATUS |

Definition at line 254 of file NAFE33352.h.

## ◆ Register24

enum class NAFE33352_Base::Register24 : uint16_t
| strong

Enumerator
GAIN_COEF0 |
GAIN_COEF1 |
GAIN_COEF2 |
GAIN_COEF3 |
GAIN_COEF4 |
GAIN_COEF5 |
GAIN_COEF6 |
GAIN_COEF7 |
OFFSET_COEF0 |
OFFSET_COEF1 |
OFFSET_COEF2 |
OFFSET_COEF3 |
OFFSET_COEF4 |
OFFSET_COEF5 |
OFFSET_COEF6 |
OFFSET_COEF7 |
EXTRA_CAL_COEF0 |
EXTRA_CAL_COEF1 |
EXTRA_CAL_COEF2 |
EXTRA_CAL_COEF3 |
EXTRA_CAL_COEF4 |
EXTRA_CAL_COEF5 |
EXTRA_CAL_COEF6 |
EXTRA_CAL_COEF7 |
SERIAL1 |
SERIAL0 |
AI_DATA0 |
AI_DATA1 |
AI_DATA2 |
AI_DATA3 |
AI_DATA4 |
AI_DATA5 |
AI_DATA6 |
AI_DATA7 |
AI_CH_OVR_THR_0 |
AI_CH_OVR_THR_1 |
AI_CH_OVR_THR_2 |
AI_CH_OVR_THR_3 |
AI_CH_OVR_THR_4 |
AI_CH_OVR_THR_5 |
AI_CH_OVR_THR_6 |
AI_CH_OVR_THR_7 |
AI_CH_UDR_THR_0 |
AI_CH_UDR_THR_1 |
AI_CH_UDR_THR_2 |
AI_CH_UDR_THR_3 |
AI_CH_UDR_THR_4 |
AI_CH_UDR_THR_5 |
AI_CH_UDR_THR_6 |
AI_CH_UDR_THR_7 |
AO_DATA |
AO_OC_POS_LIMIT |
AO_OC_NEG_LIMIT |
AWG_AMP_MAX |
AWG_AMP_MIN |

Definition at line 295 of file NAFE33352.h.

## Constructor & Destructor Documentation

## ◆ NAFE33352_Base()

NAFE33352_Base::NAFE33352_Base | ( | bool | spi_addr,
|  | bool | highspeed_variant,
|  | int | nINT,
|  | int | DRDY,
|  | int | SYN,
|  | int | nRESET,
|  | int | DRDY_input,
|  | int | SYNCDAC )

Constructor to create a NAFE33352_Base instance

Definition at line 115 of file NAFE33352.cpp.

Referenced by NAFE33352::NAFE33352(), and NAFE33352_UIOM::NAFE33352_UIOM().

## ◆ ~NAFE33352_Base()

NAFE33352_Base::~NAFE33352_Base | ( |  | ) |
| virtual

Destractor

Definition at line 127 of file NAFE33352.cpp.

## Member Function Documentation

## ◆ bit_op()

template<typename T>

uint32_t NAFE33352_Base::bit_op | ( | T | rg,
|  | uint32_t | mask,
|  | uint32_t | value )
| inline

Register bit operation

overwrite bits i a register

Parameters

  reg | register specified by Register16 or Register24 member
  mask | mask bits
  reg | value to over write

Definition at line 435 of file NAFE33352.h.

Referenced by close_logical_channel(), DRDY_by_sequencer_done(), and enable_logical_channel().

## ◆ boot()

void NAFE33352_Base::boot | ( | void |  | ) |
| virtual

Set system-level config registers

Implements AFE_base.

Definition at line 131 of file NAFE33352.cpp.

## ◆ calc_delay()

double NAFE33352_Base::calc_delay | ( | int | ch | ) |
| private

Definition at line 285 of file NAFE33352.cpp.

Referenced by open_logical_channel().

## ◆ channel_info_update()

void NAFE33352_Base::channel_info_update | ( | uint16_t | value | ) |
| private

Definition at line 260 of file NAFE33352.cpp.

Referenced by close_logical_channel(), close_logical_channel(), and enable_logical_channel().

## ◆ close_logical_channel() [1/2]

void NAFE33352_Base::close_logical_channel | ( | int | ch | ) |
| virtual

Logical channel disable

Parameters

  ch | logical channel number (0 ~ 15)

Implements AFE_base.

Definition at line 352 of file NAFE33352.cpp.

## ◆ close_logical_channel() [2/2]

void NAFE33352_Base::close_logical_channel | ( | void |  | ) |
| virtual

All logical channel disable

Implements AFE_base.

Definition at line 360 of file NAFE33352.cpp.

## ◆ command()

void NAFE33352_Base::command | ( | uint16_t | com | ) |
| virtual

Command

Parameters

  com | "Comand" type or uint16_t value

Definition at line 424 of file NAFE33352.cpp.

Referenced by boot(), calc_delay(), open_logical_channel(), reset(), start(), start(), and start_continuous_conversion().

## ◆ dac_code()

int32_t NAFE33352_Base::dac_code | ( | double | a,
|  | double | full_scale,
|  | uint8_t | bit_length )

Definition at line 412 of file NAFE33352.cpp.

Referenced by dac_out().

## ◆ dac_out()

void NAFE33352_Base::dac_out | ( | double | vi,
|  | double | full_scale,
|  | uint8_t | bit_length )
| virtual

Definition at line 407 of file NAFE33352.cpp.

## ◆ DRDY_by_sequencer_done()

void NAFE33352_Base::DRDY_by_sequencer_done | ( | bool | flag = true | ) |
| virtual

DRDY event select

Parameters

  set | true for DRDY by sequencer is done

Implements AFE_base.

Definition at line 382 of file NAFE33352.cpp.

Referenced by boot().

## ◆ enable_logical_channel()

void NAFE33352_Base::enable_logical_channel | ( | int | ch | ) |
| virtual

Logical channel enable

Parameters

  ch | logical channel number (0 ~ 15)

Implements AFE_base.

Definition at line 344 of file NAFE33352.cpp.

Referenced by open_logical_channel().

## ◆ open_dac_output()

void NAFE33352_Base::open_dac_output | ( | const uint16_t(&) | cc[6] | ) |

Definition at line 178 of file NAFE33352.cpp.

## ◆ open_logical_channel() [1/2]

void NAFE33352_Base::open_logical_channel | ( | int | ch,
|  | const uint16_t(&) | cc[4] )
| virtual

Configure logical channel

Parameters

  ch | logical channel number (0 ~ 15)
  cc | array for AI_CONFIG0, AI_CONFIG1, AI_CONFIG2 and dummy values

Implements AFE_base.

Definition at line 185 of file NAFE33352.cpp.

## ◆ open_logical_channel() [2/2]

void NAFE33352_Base::open_logical_channel | ( | int | ch,
|  | uint16_t | cc0,
|  | uint16_t | cc1,
|  | uint16_t | cc2,
|  | uint16_t | dummy )
| virtual

Configure logical channel

Parameters

  ch | logical channel number (0 ~ 15)
  cc0 | 16bit value to be set AI_CONFIG0 register (0x20)
  cc1 | 16bit value to be set AI_CONFIG1 register (0x21)
  cc2 | 16bit value to be set AI_CONFIG2 register (0x22)
  dummy | dummy variable to keep compatibility over AFE devices

Implements AFE_base.

Definition at line 337 of file NAFE33352.cpp.

Referenced by open_logical_channel().

## ◆ part_number()

uint64_t NAFE33352_Base::part_number | ( | void |  | ) |

Read part_number

Returns
  0x13388B40

Definition at line 449 of file NAFE33352.cpp.

## ◆ raw2v()

double NAFE33352_Base::raw2v | ( | int | ch,
|  | raw_t | value )
| inlinevirtual

Convert raw output to volt

Parameters

  ch | logical channel number to select its gain coefficient
  value | ADC read value

Implements AFE_base.

Definition at line 212 of file NAFE33352.h.

## ◆ read() [1/3]

int32_t NAFE33352_Base::read | ( | int | ch | ) |
| virtual

Read ADC for single channel

Parameters

  ch | logical channel number (0 ~ 15)

Implements AFE_base.

Definition at line 387 of file NAFE33352.cpp.

Referenced by read().

## ◆ read() [2/3]

void NAFE33352_Base::read | ( | raw_t * | data | ) |
| virtual

Read ADC for all channel

Parameters

  data_ptr | pointer to array to store ADC data

Implements AFE_base.

Definition at line 392 of file NAFE33352.cpp.

## ◆ read() [3/3]

void NAFE33352_Base::read | ( | volt_t * | data | ) |
| virtual

Read ADC for all channel

Parameters

  data_ptr | pointer to array to store ADC data

Implements AFE_base.

Definition at line 397 of file NAFE33352.cpp.

## ◆ reg() [1/4]

uint16_t NAFE33352_Base::reg | ( | Register16 | r | ) |
| virtual

Read register

Reads register. Register width is selected by reg type (Register16 ot Register24)

Parameters

  reg | register specified by Register16 member

Returns
  readout value

Definition at line 439 of file NAFE33352.cpp.

## ◆ reg() [2/4]

void NAFE33352_Base::reg | ( | Register16 | r,
|  | uint16_t | value )
| virtual

Write register

Writes register. Register width is selected by reg type (Register16 ot Register24)

Parameters

  reg | register specified by Register16 member

Definition at line 429 of file NAFE33352.cpp.

Referenced by bit_op(), boot(), calc_delay(), close_logical_channel(), dac_out(), open_dac_output(), open_logical_channel(), part_number(), read(), reset(), revision_number(), serial_number(), and temperature().

## ◆ reg() [3/4]

uint32_t NAFE33352_Base::reg | ( | Register24 | r | ) |
| virtual

Read register

Reads register. Register width is selected by reg type (Register16 ot Register24)

Parameters

  reg | register specified by Register24 member

Returns
  readout value

Definition at line 444 of file NAFE33352.cpp.

## ◆ reg() [4/4]

void NAFE33352_Base::reg | ( | Register24 | r,
|  | uint32_t | value )
| virtual

Write register

Writes register. Register width is selected by reg type (Register16 ot Register24)

Parameters

  reg | register specified by Register24 member

Definition at line 434 of file NAFE33352.cpp.

## ◆ reset()

void NAFE33352_Base::reset | ( | bool | hardware_reset = false | ) |
| virtual

Issue RESET command

Implements AFE_base.

Definition at line 147 of file NAFE33352.cpp.

## ◆ revision_number()

uint8_t NAFE33352_Base::revision_number | ( | void |  | ) |

Read rivision number

Returns
  PN0 register value & 0xF

Definition at line 454 of file NAFE33352.cpp.

## ◆ serial_number()

uint64_t NAFE33352_Base::serial_number | ( | void |  | ) |

Read serial number

Returns
  serial number

Definition at line 459 of file NAFE33352.cpp.

Referenced by serial_number().

## ◆ start() [1/2]

void NAFE33352_Base::start | ( | int | ch | ) |
| virtual

Start ADC

Parameters

  ch | logical channel number (0 ~ 15)

Implements AFE_base.

Definition at line 366 of file NAFE33352.cpp.

## ◆ start() [2/2]

void NAFE33352_Base::start | ( | void |  | ) |
| virtual

Start ADC on all logical channel

Implements AFE_base.

Definition at line 372 of file NAFE33352.cpp.

## ◆ start_continuous_conversion()

void NAFE33352_Base::start_continuous_conversion | ( | void |  | ) |
| virtual

Start continuous AD conversion

Implements AFE_base.

Definition at line 377 of file NAFE33352.cpp.

## ◆ temperature()

float NAFE33352_Base::temperature | ( | void |  | ) |

Die temperature

Returns
  die temperature in celsius

Definition at line 468 of file NAFE33352.cpp.

## Member Data Documentation

## ◆ dac

DAC NAFE33352_Base::dac

Definition at line 143 of file NAFE33352.h.

Referenced by NAFE33352_Base().

## ◆ logical_channel

LogicalChannel NAFE33352_Base::logical_channel[16]

16 LogicalChannel instance array

Definition at line 74 of file NAFE33352.h.

Referenced by NAFE33352_Base().

## ◆ on_board_shunt_resister

double NAFE33352_Base::on_board_shunt_resister = 50.00
| staticconstexpr

Definition at line 20 of file NAFE33352.h.

Referenced by raw2v().

## ◆ pga_gain

double NAFE33352_Base::pga_gain[] = { 1.00, 16.00 }
| staticconstexpr

Definition at line 225 of file NAFE33352.h.

The documentation for this class was generated from the following files:

- NAFE33352.h
- NAFE33352.cpp