AFE_NXP_Arduino 2.0.0 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
NAFE13388_7_0_LoadCell Directory Reference

## Detailed Description

# 7_0_NAFE13388_LoadCell

Practical sample to measure loadcell output using internal voltage excitation source.

This sample uses 1 logical channel.
The logical channel setting defines analog input channel selections as well as excitation current configurations.

# Wiring

# Logical channel setting on channel 0