AFE_NXP_Arduino 2.0.0 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
AFE_base Member List

This is the complete list of members for AFE_base, including all inherited members.

AFE_base(bool spi_addr, bool highspeed_variant, int nINT, int DRDY, int SYN, int nRESET, int DRDY_input, int SYNCDAC) | AFE_base |
begin(void) | AFE_base | virtual
bit_count(uint32_t value) | AFE_base | protected
boot(void)=0 | AFE_base | pure virtual
burst(uint32_t *data, int length, int width=3) | SPI_for_AFE |
callback_fp_t typedef | AFE_base |
cbf_DRDY | AFE_base | protectedstatic
ch_delay | AFE_base | protected
close_logical_channel(int ch)=0 | AFE_base | pure virtual
close_logical_channel(void)=0 | AFE_base | pure virtual
coeff_V | AFE_base | protected
command_length | SPI_for_AFE | privatestatic
default_drdy_cb() | AFE_base | protected
delay_accuracy | AFE_base | protectedstatic
dev_add | AFE_base | protected
DRDY_by_sequencer_done(bool flag=true)=0 | AFE_base | pure virtual
DRDY_cb() | AFE_base | protectedstatic
drdy_count | AFE_base | protected
drdy_delay(int ch) | AFE_base | inline
drdy_delay(void) | AFE_base | inline
drdy_flag | AFE_base | protected
enable_logical_channel(int ch)=0 | AFE_base | pure virtual
enabled_channels | AFE_base | protected
enabled_logical_channels(void) | AFE_base | inline
get_data16(uint8_t *vp) | SPI_for_AFE | inlineprivate
get_data24(uint8_t *vp) | SPI_for_AFE | inlineprivate
GPIO0_GPIO1 enum value | AFE_base |
highspeed_variant | AFE_base | protected
HV_MUX enum value | AFE_base |
init(void) | AFE_base | protectedvirtual
instance | AFE_base | static
LV_mux_sel enum name | AFE_base |
mux_setting | AFE_base | protected
open_logical_channel(int ch, uint16_t cc0, uint16_t cc1, uint16_t cc2, uint16_t cc3)=0 | AFE_base | pure virtual
open_logical_channel(int ch, const uint16_t(&cc)[4])=0 | AFE_base | pure virtual
pin_DRDY | AFE_base | protected
pin_DRDY_input | AFE_base | protected
pin_nINT | AFE_base | protected
pin_nRESET | AFE_base | protected
pin_SYN | AFE_base | protected
pin_SYNCDAC | AFE_base | protected
raw2mv(int ch, raw_t value) | AFE_base | inline
raw2uv(int ch, raw_t value) | AFE_base | inline
raw2v(int ch, raw_t value)=0 | AFE_base | pure virtual
raw_t typedef | AFE_base |
read(int ch)=0 | AFE_base | pure virtual
read(raw_t *data_ptr)=0 | AFE_base | pure virtual
read(volt_t *data_ptr)=0 | AFE_base | pure virtual
read_r16(uint16_t reg) | SPI_for_AFE |
read_r24(uint16_t reg) | SPI_for_AFE |
REF2_REF2 enum value | AFE_base |
REF2_VHSS enum value | AFE_base |
REFCOARSE_REF2 enum value | AFE_base |
reset(bool hardware_reset=false)=0 | AFE_base | pure virtual
sequence_order | AFE_base | protected
set_DRDY_callback(callback_fp_t fnc) | AFE_base | virtual
start(int ch)=0 | AFE_base | pure virtual
start(void)=0 | AFE_base | pure virtual
start_and_read(int ch) | AFE_base | virtual
start_and_read(T data) | AFE_base | inline
start_continuous_conversion(void)=0 | AFE_base | pure virtual
static_default_drdy_cb() | AFE_base | protectedstatic
timeout_limit | AFE_base | protectedstatic
total_delay | AFE_base | protected
txrx(uint8_t *data, int size) | SPI_for_AFE |
use_DRDY_trigger(bool use=true) | AFE_base |
VADD_REF2 enum value | AFE_base |
VHDD_REF2 enum value | AFE_base |
volt_t typedef | AFE_base |
wait_conversion_complete(double delay=-1.0) | AFE_base | protected
write_r16(uint16_t reg) | SPI_for_AFE |
write_r16(uint16_t reg, uint16_t val) | SPI_for_AFE |
write_r24(uint16_t reg, uint32_t val) | SPI_for_AFE |
~AFE_base() | AFE_base | virtual